For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the speaker. Refer to Radio Front Side Door Lower Speaker Replacement .
3. Remove the water deflector. Refer to Front Side Door Water Deflector Replacement .
4. Remove the window regulator. Refer to Front Side Door Window Regulator Replacement .
5. Remove the window regulator motor to window regulator retaining bolts (1).
6. Remove the window regulator motor (2) from the window regulator (1).

### Installation Procedure

1. Position the window regulator motor (2) to the window regulator (1).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the window regulator motor to window regulator retaining bolts (1).

Tighten
Tighten the bolts to 8 N-m (71 lb in).

3. Install the window regulator. Refer to Front Side Door Window Regulator Replacement .
4. Install the water deflector. Refer to Front Side Door Water Deflector Replacement .
5. Install the speaker. Refer to Radio Front Side Door Lower Speaker Replacement .
6. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement .