For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Condenser to Radiator Retaining Bolt | 11 N·m | 97 lb in
Coolant Air Bleed Hose Retaining Clamp | 4 N·m | 35 lb in
Coolant Air Bleed Pipe Retaining Bolts | 12 N·m | 106 lb in
Coolant Inlet Pipe to Alternator Bracket Retaining Nut - 3.6L | 25 N·m | 18 lb ft
Coolant Recovery Reservoir Retaining Nuts | 17 N·m | 13 lb ft
Cooling Fan Blade Retaining Nut | 6 N·m | 53 lb in
Cooling Fan Motor to Fan Shroud Bolt | 10 N·m | 89 lb in
Coolant Inlet Pipe Retaining Bolt | 35 N·m | 26 lb ft
Heater Pipe Assembly to Thermostat Housing Retaining Bolts - 3.6L | 10 N·m | 89 lb in
Radiator Cap | 5 N·m | 44 lb in
Radiator Drain Plug | 2 N·m | 18 lb in
Thermostat Housing Retaining Bolts - 6.0L | 14 N·m | 124 lb in
Thermostat Housing to Cylinder Block Retaining Bolts - 3.6L | 10 N·m | 89 lb in

- Water Pump to Engine Front Cover Retaining Bolts - 3.6

10 N·m

89 lb in

- Water Pump Pulley to Water Pump Retaining Bolts - 3.6

10 N·m

89 lb in

Water Pump Retaining Bolts - 6.0L | 25 N·m | 18 lb ft

- First Pass

15 N·m

11 lb ft

- Final Pass

25 N·m

18 lb ft