For 1990-2009 cars

### Removal Procedure

Important: Carefully remove the roof drip moulding, failure to do so will result in damage to the roof drip moulding.

1. Open the front and rear doors of the vehicle on the relevant side.

Important: Take care not to damage the paint on the vehicle when prying the roof drip moulding from the vehicle.

2. Use a suitable tool to carefully remove the roof drip moulding, starting from the front of the vehicle, by prying the roof drip moulding retaining clips (1) away from the vehicle.
3. Remove the roof drip moulding (2) from the vehicle.

### Installation Procedure

1. Clean the roof drip gutter with a suitable cleaning solution, using a lint free cloth.
2. Install the roof drip moulding (1) starting at the rear of the moulding.

Important: Make sure that the rear datum pin is secure and in the correct position.

3. Install the body side roof drip moulding (1) rear datum pin (2) to the vehicle.
4. Install the remaining roof drip moulding retaining clips (1) working from the rear to the front of the vehicle.
5. Close the front and rear doors of the vehicle on the relevant side.