For 1990-2009 cars

### Removal Procedure - Manual Day/Night Adjustment

Important: The rearview mirror boss (1) is not serviced separately and is part of the windshield assembly.

1. Detach the rearview mirror (2) from the windshield mirror boss (1) by firmly pulling downward.
2. Detach the rearview mirror (2) from the windshield mirror boss (1).

### Installation Procedure - Manual Day/Night Adjustment

1. Slide the rearview mirror (2) downwards on the rearview mirror boss (1) until an audible click noise is heard.
2. Install the rearview mirror (2) to the rearview mirror boss (1).

### Removal Procedure - Electro-chromatic

Important: Remove the rearview mirror wiring harness cover (1) by sliding it upwards and outwards.

1. Remove the rearview mirror wiring harness cover (1) from the rearview mirror (2).
2. Disconnect the rearview mirror electrical connector (1) from the rearview mirror (2).

Important: Detach the rearview mirror (2) from the rearview mirror boss (1) by firmly pulling downward.

Important: The rearview mirror boss (1) is not serviced separately and is part of the windshield assembly.

3. Detach the rearview mirror (2) from the windshield mirror boss (1).
4. Remove the rearview mirror (2) from the vehicle.

### Installation Procedure - Electro-chromatic

Important: Slide the rearview mirror (2) downwards on the rearview mirror boss (1) until an audible click noise is heard.

1. Install the rearview mirror (2) to the rearview mirror boss (1).
2. Connect the rearview mirror electrical connector (1) to the rearview mirror (2).

Important: Install the rearview mirror cover (1) by sliding it inwards and downwards.

3. Install the rearview mirror wiring harness cover (1) to the rearview mirror (2).

### Removal Procedure - Telematic

Important: Remove the rearview mirror wiring harness cover (1) by sliding it upwards and outwards.

1. Remove the rearview mirror wiring harness cover (1) from the rearview mirror (2).

Important: The rearview mirror boss is not serviced separately and is part of the windshield assembly.

2. Remove the rearview mirror retaining screw (2) from the rearview mirror (1).
3. Disconnect the rearview mirror electrical connector (2) from the rearview mirror (1).

Important: Remove the rearview mirror (2) by sliding it upwards.

4. Remove the rearview mirror (2) from the rearview mirror boss (1).

### Installation Procedure - Telematic

Important: Slide the rearview mirror (2) downwards on the rearview mirror boss (1).

1. Install the rearview mirror (2) to the rearview mirror boss (1).
2. Connect the rearview mirror electrical connector (2) to the rearview mirror (1).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the rearview mirror retaining screw (2) to the rearview mirror (1).

Tighten
Tighten the screw to 4 N-m (35 lb in).

Important: Install the rearview mirror cover (1) by sliding it inwards and downwards.

4. Install the rearview mirror wiring harness cover (1) to the rearview mirror (2).