For 1990-2009 cars

## Fastener Tightening Specifications LWB SWB

Application | Specification
--- | ---
Metric | English
Front Air Deflector to Front Fascia Retaining Screws | 3 N·m | 27 lb in
Front Bumper Fascia to Fender Retaining Bolts | 10 N·m | 89 lb in
Front Bumper Impact Bar to Chassis Retaining Bolts | 22 N·m | 16 lb ft
Front Bumper Impact Bar to Front End Module Retaining Bolts | 4 N·m | 35 lb in
Front Energy Absorber to Front End Module Retaining Bolts | 4 N·m | 35 lb in
Front Fascia Bracket Retaining Bolts | 4 N·m | 35 lb in
Radiator Grille to Front End Module Retaining Bolts | 4 N·m | 35 lb in
Rear Bumper Bracket to Rear Compartment Floor Retaining Bolts | 58 N·m | 43 lb ft
Rear Impact Bar Retaining Nuts | 22 N·m | 16 lb ft
Rear Bumper Fascia to Rear End Panel Retaining Screws | 2 N·m | 18 lb in
Rear Fascia Extension Retaining Screws | 2 N·m | 18 lb in
Rear Fascia to Rear Fascia Reflector Retaining Screw | 2 N·m | 18 lb in