For 1990-2009 cars

## Driver Seat Adjuster Memory Switch Replacement LHD

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the battery ground cable from the battery. Refer to Battery Negative Cable Disconnection and Connection .

Caution: Refer to SIR Caution in the Preface section.

2. Disable the SIR system. Refer to SIR Disabling and Enabling in SIR.
3. Remove the front seat. Refer to Front Seat Replacement - Bucket .
4. Remove the outer trim panel. Refer to Seat Cushion Outer Trim Panel Replacement .
5. Disconnect the memory switch electrical connector (1).
6. Remove screw (4) attaching the memory position switch (2) to the front seat outer side cover (3).
7. Lift out the memory position switch (2) from its recess in the side cover (3).
8. As required, each position switch button can be removed from the switch.

### Installation Procedure

Important: Ensure buttons are installed as per removal.

1. As required, install the position button by pushing it into the memory position switch, listen for an audible click to confirm fitting
2. Install the seat memory position switch (2), into the its recess in the outer seat trim (3).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the memory position switch retaining screw (4).

Tighten
Tighten the screw to 2.0 N·m (18 lb in).

4. Connect the memory switch electrical connector (1).
5. Install the outer trim panel. Refer to Seat Cushion Outer Trim Panel Replacement .
6. Install the front seat. Refer to Front Seat Replacement - Bucket .

Caution: Refer to Fastener Notice in the Preface section.

7. Enable the SIR system. Refer to SIR Disabling and Enabling in SIR.
8. Connect the battery ground cable to the battery. Refer to Battery Negative Cable Disconnection and Connection .
9. Test the seat for correct mechanical and electrical operation.