For 1990-2009 cars

### Removal Procedure

1. Remove front bumper. Refer to Front Bumper Fascia Replacement.

Important: To remove the ambient temperature sensor (1) squeeze the locking tabs (3) and push free from the bracket.

2. Detach the ambient air temperature sensor (1) from the bracket.
3. Disconnect the ambient temperature sensor electrical connector (2).
4. Remove the ambient air temperature sensor (1).

### Installation Procedure

1. Connect the ambient temperature sensor electrical connector (2).

Important: Make sure that the locking tabs (3) and are correctly located.

2. Install the ambient temperature sensor (1) to the bracket.
3. Install the front bumper fascia. Refer to Front Bumper Fascia Replacement.