For 1990-2009 cars

## Cylinder Head Removal - Left Side LLT

1. Remove the two front M8 left cylinder head bolts.
2. Remove the left cylinder head bolts.
3. Remove the left cylinder head.
4. Remove and discard the left cylinder head gasket.

## Cylinder Head Removal - Left Side LY7

1. Remove the left bank cylinder head to cylinder block retaining bolts (1 and 2).
2. Remove the left bank cylinder head (3).
3. Remove and discard the left cylinder head gasket (1).