For 1990-2009 cars

#### Inflation Pressure Conversion (Kilopascals to Psi)

Refer to the Tyre Placard located on the B pillar of the vehicle for the correct tyre inflation pressure and load for the factory installed tyres. The tyre pressures may be printed in both kilopascal (kPa) and psi. The correct tyre inflation pressures for the factory installed tyres is when the tyres are cold. "Cold" means the vehicle has been sitting for at least 3 hours or driven no more than 1.6 km (1 mi). Inspect the tyres inflation pressure when the tyres are cold. One psi equals 6.9 kPa.
kPa | psi | kPa | psi
--- | --- | --- | ---
140 | 20 | 215 | 31
145 | 21 | 220 | 32
155 | 22 | 230 | 33
160 | 23 | 235 | 34
165 | 24 | 240 | 35
170 | 25 | 250 | 36
180 | 26 | 275 | 40
185 | 27 | 310 | 45
190 | 28 | 345 | 50
200 | 29 | 380 | 55
205 | 30 | 415 | 60
Conversion: 6.9 kPa=1 psi