For 1990-2009 cars

## Camshaft Cover Removal - Left Side LLT

1. Remove the ignition coil bolts.
2. Remove the ignition coils.
3. Remove the left camshaft cover bolts.
4. Remove and discard the camshaft cover grommets and camshaft cover bolts if they are serviced with the grommet.
5. Remove the left camshaft cover from the left cylinder head.

## Camshaft Cover Removal - Left Side LY7

1. Remove the ignition coil to camshaft cover retaining bolts (1).
2. Remove the ignition coils (2) from the camshaft cover (3).
3. Remove the spark plugs (1).
4. Remove the camshaft cover to cylinder head retaining bolts (1).
5. Remove the camshaft cover (2) from the cylinder head (3).

Important: The camshaft cover seal and grommets must be discarded whenever the camshaft cover has been removed from the cylinder head (2).

6. Remove the camshaft cover seal and grommets.

Discard the seal and grommets