For 1990-2009 cars

#### Tools Required

• | EN-46103 Camshaft Actuator Valve Seal Remover/Installer

• | J 29184 Oil Seal Installer

Important: DO NOT lubricate the crankshaft front oil seal or crankshaft balancer sealing surfaces. The crankshaft balancer is installed into a dry seal.

1. Install the NEW crankshaft front oil seal into the engine front cover using the J 29184 .
2. Install the NEW camshaft position actuator solenoid seals into the engine front cover using the EN-46103 .