For 1990-2009 cars

### Removal Procedure

Caution: Refer to Glass and Sheet Metal Handling Caution in the Preface section.

Caution: Refer to Express Window Down Caution in the Preface section.

1. Remove the door trim panel. Refer to Rear Side Door Trim Panel Replacement.
2. Remove the rear sunshade. Refer to Sunshade Replacement.
3. Remove the speaker. Refer to Radio Rear Side Door Speaker Replacement.
4. Remove the water deflector. Refer to Rear Side Door Water Deflector Replacement.
5. Remove the window inner belt sealing strip. Refer to Rear Side Door Window Inner Sealing Strip Replacement.
6. Remove the rear door stationary window. Refer to Rear Side Door Window Frame Rear Applique Replacement.
7. Remove the window inner weatherstrip. Refer to Rear Side Door Window Inner Weatherstrip Replacement.
8. Remove the window outer belt sealing strip. Refer to Rear Side Door Window Outer Sealing Strip Replacement.
9. Remove the window inner sealing strip. Refer to Rear Side Door Window Inner Sealing Strip Replacement.
10. Raise and support the window to the full up position.

Important: With the aid of an assistant hold the window while the support is removed.

11. Loosen the window regulator to window retaining bolts (1).
12. Lower the window regulator approximately 1/2 way down.
13. Remove the support from the window.

Important: Remove the window (1) with the aid of an assistant.

14. Remove the window (1) up and out of the door assembly (2).

### Installation Procedure

Important: Install the window (1) with the aid of an assistant.

Important: The window regulator should be approximately 1/2 way down before installing the window (1).

1. Install the window (1) down into the door assembly (2).
2. Lower the window into the window clamps.
3. Lower the window.
4. Install the inner window weatherstrip. Refer to Rear Side Door Window Inner Weatherstrip Replacement.
5. Install the rear door stationary window. Refer to Rear Side Door Window Frame Rear Applique Replacement.
6. Install the window inner sealing strip. Refer to Rear Side Door Window Inner Sealing Strip Replacement.
7. Start the vehicle in order to make sure maximum power to the window motor. This is required to fully seat the window for adjustment.
8. Raise the window to full up position.

Notice: Refer to Fastener Notice in the Preface section.

9. Tighten the window regulator to window retaining bolts (1).

Tighten
Tighten the nuts to 8 N-m (71 lb in).

10. Inspect the window for correct operation and a tight seal.
11. Shut off the vehicle.
12. Install the window outer belt sealing strip. Refer to Rear Side Door Window Outer Sealing Strip Replacement.
13. Install the window inner belt sealing strip. Refer to Rear Side Door Window Inner Sealing Strip Replacement.
14. Install water deflector. Refer to Rear Side Door Water Deflector Replacement.
15. Install the speaker. Refer to Radio Rear Side Door Speaker Replacement in Entertainment.
16. Install the rear sunshade. Refer to Sunshade Replacement.
17. Install the door trim panel. Refer to Rear Side Door Trim Panel Replacement.