For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to General Repair Instructions in the Preface section. Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Place a suitable drain pan under the transmission.

1 | Transmission Fluid Pan Bolt (Qty: 18) Tip Tighten the bolts in the sequence shown. Tighten 9 N·m (80 lb. in)
2 | Transmission Fluid Pan Assembly

• | Check the condition of the draining fluid. Refer to Transmission Fluid Check .

• | Fill the transmission with the proper fluid. Refer to Transmission General Specifications .

• | Fill the transmission with the proper amount of transmission fluid. Refer to Fluid Capacity Specifications and Transmission Fluid Check .

3 | Transmission Fluid Pan Gasket Tip The fluid pan gasket is reusable. Inspect the gasket to determine if it may be reused.
4 | NEW Fluid Filter Assembly Tip Pull the fluid filter assembly straight out. Do not bend or twist the filter neck.
5 | NEW Fluid Filter Seal Assembly Notice: Refer to Fastener Notice in the Preface section. Notice: Refer to General Repair Instructions in the Preface section.

• | Use a screwdriver or snap ring pliers to remove the filter seal.

• | Use the DT 47848 and the J 42183 to install the filter seal.

• | Lubricate the filter seal with transmission fluid before installing the filter.

6 |

• | DT 47848 .

• | J 42183 .