For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Exhaust Manifold to Cylinder Head Retaining Bolts - 3.6L Engine | 20 N·m | 15 lb ft
Exhaust Manifold Heat Shield to Exhaust Manifold Retaining Bolts - 3.6L Engine | 10 N·m | 89 lb in
Catalytic Converter to Exhaust Manifold Retaining Nuts - 3.6L Engine | 45 N·m | 33 lb ft
Intermediate Exhaust Assembly to Catalytic Converter Retaining Nuts | 40 N·m | 30 lb ft
Rear Muffler to Intermediate Exhaust Assembly Retaining Nuts | 45 N·m | 33 lb ft
Centre Insulator Hanger Bracket to Differential Retaining Bolt | 45 N·m | 33 lb ft
Rear Insulator Hanger Bracket to Body Retaining Bolts | 26 N·m | 19 lb ft
Front Exhaust Foil Heat Shield to Body Retaining Bolt | 4 N·m | 35 lb in
Centre Exhaust Heat Shield to Body Retaining Bolts | 4 N·m | 35 lb in
Exhaust Muffler Heat Shield to Body Retaining Bolts | 4 N·m | 35 lb in
Fuel Tank Heat Shield to Fuel Tank Retaining Nuts | 4 N·m | 35 lb in
Exhaust Manifold Heat Shield to Exhaust Manifold Retaining Bolts | 10 N·m | 89 lb in