For 1990-2009 cars

## Rear Wheel Bearing and Hub Replacement Original

### Removal Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

1. Remove the wheel hub and knuckle assembly. Refer to Knuckle Replacement.
2. Secure the wheel hub and knuckle assembly using a suitable vice.
3. Remove the wheel speed sensor to knuckle retaining bolt (2).
4. Remove the wheel speed sensor (1).

Important: The wheel bearing will be damaged when pressing out the wheel hub flange. The wheel bearing must be replaced every time the wheel hub is removed.

5. Remove the wheel hub flange using a suitable workshop press.
6. Remove the park brake shoes. Refer to Parking Brake Shoe Replacement.
7. Remove the disc brake backing plate to knuckle retaining bolts (3 and 4).
8. Remove the disc brake backing plate (2) from the knuckle (1).
9. Remove the wheel bearing retaining circlip (3) using suitable circlip pliers.

Important: The wheel bearing will be damaged when pressing out the wheel hub flange. The wheel bearing must be replaced every time the wheel hub is removed.

10. Press the wheel bearing (2) from the knuckle (1) using a suitable workshop press.

Discard the wheel bearing.

### Installation Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

Important: Prior to installing the NEW wheel bearing it is essential that the correct orientation is attained, the wheel speed sensor decoder ring MUST face inboard, towards the wheel speed sensor. Failure to install in the correct orientation will result in ABS/ESP faults.

1. Install the NEW wheel bearing (2) to the knuckle (1) using a workshop press.
2. Install the wheel bearing retaining circlip (3) using suitable circlip pliers.
3. Install the disc brake backing plate (2) to the knuckle (1).

Notice: Refer to Fastener Notice in the Preface section.

4. Install the upper disc brake backing plate to knuckle retaining bolt (3).

Tighten
Tighten the bolts to 60 Nm (44 lb ft).

5. Install the lower disc brake backing plate to knuckle retaining bolts (4).

Tighten
Tighten the bolts to 130 Nm (96 lb ft).

6. Install the park brake shoes. Refer to Parking Brake Shoe Replacement.

Important: The wheel hub flange (1) must be fully seated against the wheel bearing.

7. Install the wheel hub flange (1) using a suitable press.
8. Install the wheel speed sensor (1).

Notice: Refer to Fastener Notice in the Preface section.

9. Install the wheel speed sensor to knuckle retaining bolt (2).

Tighten
Tighten the bolt to 7 N·m (62 lb in).

10. Remove the hub and knuckle assembly from the vice.
11. Install the wheel hub and knuckle assembly. Refer to Knuckle Replacement.