For 1990-2009 cars

1. Remove the transmission. Refer to Transmission Replacement.
2. Rotate the transmission 90 degrees so that the converter housing is facing up. Remove the torque converter housing bolts (2) from the torque converter housing (3).
3. Remove the torque converter housing assembly (3) from the case (24).
4. Remove the torque converter housing fluid seal assembly (4).
5. Remove the fluid pump cover gasket (46).