For 1990-2009 cars

Table 1: | Upper to Lower Control Valve Body Assemblies Assemble
Table 2: | Filter Plate Installation
Table 3: | Control Solenoid Valve Assembly Installation
Table 4: | Manual Shift Shaft Position Switch Installation
Table 5: | Valve Body, Control Solenoid Torque Sequence
Table 6: | Control Solenoid Valve Assembly Contact Gap Inspection
Table 7: | Input and Output Speed Sensor Assembly Installation

### Upper to Lower Control Valve Body Assemblies Assemble

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .
1 | Control Valve Body Ball Check Valve (Quantity: 7) Tip Refer to Ball Check Valve Locations.
2 | Control Valve Body Spacer (w/Gasket) Plate Assembly Notice: Refer to General Repair Instructions in the Preface section.
3 | Control Valve Lower Body Assembly Tip Turn the valve body assembly over after installing to upper body.
4 | Bolt M5 x 36 (Quantity: 12) Tighten Tighten the bolts in the sequence shown to 8 N·m (71 lb. in).

### Filter Plate Installation

Callout | Component Name
--- | ---
1 | Filter Plate Assembly Notice: Refer to General Repair Instructions in the Preface section. Notice: Refer to General Repair Instructions in the Preface section. Tip Use care when removing or installing the filter plate assembly. However, if a retaining tab is broken or missing, DO NOT replace the control solenoid valve assembly. The filter plate assembly can still be adequately aligned.

### Control Solenoid Valve Assembly Installation

Callout | Component Name
--- | ---
1 | Control Solenoid (w/Body and TCM) Valve Assembly Tip Note the locator pin on the control valve lower body assembly while aligning the control solenoid valve assembly.
2 | Bolt M5 x 53 (Quantity: 2) Tip Hand tighten only.
3 | Bolt M5 x 55 (Quantity: 4) Tip Hand tighten only.
4 | Bolt M5 x 45 (Quantity: 5) Tip Hand tighten only.

### Manual Shift Shaft Position Switch Installation

Callout | Component Name
--- | ---
1 | A/Trans Manual Shift Shaft Position Switch Assembly
2 | Manual Valve Link Tip Align the switch activator slide with the manual valve link.
3 | Bolt M5 x 55 Tip Hand tighten only.
4 | A/Trans Manual Shift Shaft Position Switch Harness Clip Tip The wiring harness clip on the manual shift shaft position switch does not need to be replaced if damaged or missing. The clip functions only as a manufacturing assembly aid to keep the harness clear during an automated bolt installation process. If the clip is damaged, simply remove and discard.
5 | A/Trans Manual Shift Shaft Position Switch Electrical Connector Tip Connect and lock the manual shift shaft position switch electrical connector to the control solenoid valve assembly.

### Valve Body, Control Solenoid Torque Sequence

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications . Notice: Refer to General Repair Instructions in the Preface section. Tip

1. Hand tighten the last 6 bolts before final torque sequence.
2. The 2 "heat sink" bolts must be tightened last.

1 | Bolts M5 x 45 (Quantity: 5)
2 | Bolt M5 x 55 Tighten Tighten all 18 bolts in the sequence shown to 8 N·m (71 lb. in).

### Control Solenoid Valve Assembly Contact Gap Inspection

Callout | Component Name
--- | ---
1 | Control Solenoid (w/Body and TCM) Valve Assembly Tip Inspect the contact area between the "heat sink" area of the control solenoid valve assembly and the valve body. There should be no visible gap. If a gap exists, loosen all 18 bolts and retighten in the required sequence.

### Input and Output Speed Sensor Assembly Installation

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .
1 | A/Trans Input and Output Speed Sensor Wiring Harness Clip (Quantity: 2) Tip Inspect the 2 wiring harness clips for damage. Replace if damaged.
2 | A/Trans Input and Output Speed Sensor Assembly
3 | Bolt M6 x 20 (Quantity: 2) Tighten Tighten bolts to 12 N·m (106 lb. in)