For 1990-2009 cars

Gear | Shift SOL 1 | Shift SOL 2 | 1-2-3-4 CL PC SOL 5 N.L. | 2-6 CL PC SOL 4 N.L. | 3-5 REV CL PC SOL 2 N.H. | LOW REV 4-5-6 CL PC SOL 3 N.H. | Gear Ratio
--- | --- | --- | --- | --- | --- | --- | ---
Park | ON | ON | OFF | OFF | OFF | ON | --
Reverse | ON | OFF | OFF | OFF | ON | ON | 3.06
Neutral | ON | ON | OFF | OFF | OFF | ON | --
1st Braking | ON | ON | ON | OFF | OFF | ON | 4.03
1st | OFF | ON | ON | OFF | OFF | OFF | 4.03
2nd | OFF | ON | ON | ON | OFF | OFF | 2.36
3rd | OFF | ON | ON | OFF | ON | OFF | 1.53
4th | OFF | ON | ON | OFF | OFF | ON | 1.15
5th | OFF | ON | OFF | OFF | ON | ON | 0.85
6th | OFF | ON | OFF | ON | OFF | ON | 0.67
For shift solenoids 1 and 2, "ON" = Solenoid Energized (Pressurized) "OFF" = Solenoid De-energised (No Pressure). For pressure control solenoids, "ON" = Pressurized, "OFF" = No Pressure