For 1990-2009 cars

## Stationary Window Description LWB

The windshield assembly is manufactured from laminated glass and has a tinted upper band. Toughened safety glass is used for all other windows. The windshield and rear window are retained to the body with urethane adhesive which adheres the windshield and rear window to the body, increasing structural integrity. The reinstallation of the windshield and rear window with urethane adhesive requires complete replacement of the urethane adhesive bead. The quarter window assembly is attached to the vehicle using micro-encapsulated nuts.