For 1990-2009 cars

#### Tools Required

• | EN 46109 Guide Pin Set

• | EN-47839 Crankshaft Rear Oil Seal Installation Tool

• | J 42183 Handle

1. Install the 6 mm (0.236 in) guides from the EN 46109 into the 2 crankshaft rear oil seal housing corner bolt holes of the cylinder block.
2. Install the J 42183 (1) with the EN-47839 (2) onto the rear of the crankshaft flange.
3. Place a 3 mm (0.118 in) bead of RTV sealant (1) to the NEW crankshaft rear oil seal housing as shown.

Important: DO NOT allow any engine oil on the area where the crankshaft rear oil seal housing is to be installed.

4. Install the crankshaft rear oil seal housing to the cylinder block.
5. Remove the EN 46109 mm (0.236 in) guides from the cylinder block.

Notice: Refer to Fastener Notice in the Preface section.

6. Install the crankshaft rear oil seal housing to cylinder block retaining bolts.
7. Tighten the crankshaft rear oil seal housing bolts in sequence.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

8. Remove the J 42183 (1) and EN-47839 (2) from the crankshaft flange.