For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the propeller shaft. Refer to Propeller Shaft Replacement .
3. Support the transmission with a suitable jack.
4. Remove the transmission mount assembly. Refer to Transmission Mount Replacement .
5. Remove the transmission extension housing assembly. Refer to Output Shaft Seal Replacement .

1 | Output Shaft Seal

• | Use the J 45000 to remove the seal. Use care in order to avoid damaging the output shaft bushing.

• | Lubricate the seal with clean transmission fluid.

• | Use the J 38693 to install the seal.