For 1990-2009 cars

### Removal Procedure

1. Remove the outside rearview mirror. Refer to Power Mirror Replacement.
2. Lower the window to the full down position.

Important: Pull the front door outer belt sealing strip (1) to detach the retainers.

3. Remove the front door outer belt sealing strip (1) from the door (2).

### Installation Procedure

Important: Push the front door outer belt sealing strip (1) to attach the retainers.

1. Install the front door outer belt sealing strip (1) to the door (2).
2. Install the outside rearview mirror. Refer to Power Mirror Replacement.