For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Install the clutch assembly into a hole in the workbench
2. Zero out the dial indicator on the DT 47868-1 .

#### Special Tools

• | DT 47868-1 Pack Travel Weight

• | J 8001 Dial Indicator Set

• | J 26900-13 Magnetic Base

1 | 4-5-6 Clutch Apply Passage Tip While using one finger to block the top passage hole on the turbine shaft, apply compressed air to the opposite top passage hole, and observe the dial indicator measurement. Refer to Clutch Backing Plate Retaining Ring Specifications to determine the correct retainer.