For 1990-2009 cars

### Removal Procedure

1. Remove the radiator assembly. Refer to Radiator Replacement.
2. Disconnect the washer fluid level switch electrical connector (1).
3. Place a suitable container under the washer fluid level switch (2).
4. Remove the washer fluid level switch (2) from the washer fluid container and discard the rubber seal.

### Installation Procedure

Important: Insert the washer fluid level switch into the washer fluid container until fully seated.

1. Install the washer fluid level switch (2) into the washer fluid container.
2. Connect the washer fluid level switch electrical connector (1).
3. Fill the washer solvent container with washer solvent.
4. Install the radiator assembly. Refer to Radiator Replacement.