For 1990-2009 cars

Notice: Refer to Fastener Notice in the Preface section.

1. Install the oil pressure sender (1).

Tighten
Tighten the oil pressure sender to 20 N·m (15 lb in).

2. Install the NEW oil filter cartridge (1).

Notice: Refer to General Repair Instructions in the Preface section.

3. Lubricate the oil filter cap threads with clean engine oil.
4. Install the oil filter cap (1).

Tighten
Tighten the oil filter cap to 25 N·m (18 lb in).