For 1990-2009 cars

## Temperature Valve Actuator Replacement - Left Side LHD

### Removal Procedure

1. Remove the left closeout panel. Refer to Instrument Panel Extension Replacement.
2. Disconnect the left air temperature actuator electrical connector (1) from the actuator (2).
3. Remove the left air temperature actuator screws (3).
4. Remove the left air temperature actuator (1).

### Installation Procedure

1. Install the left air temperature actuator (1).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the left air temperature actuator to HVAC unit retaining screws (3).

Tighten
Tighten the screws to 1 N·m (9 lb in).

3. Connect the left air temperature actuator electrical connector (1) to the air temperature actuator (2).
4. Install the left closeout panel. Refer to Instrument Panel Extension Replacement.