For 1990-2009 cars

## Instrument Cluster Replacement LWB

### Removal Procedure

1. Remove the knee Bolster. Refer to Knee Bolster Replacement.
2. Remove the upper steering wheel cover. Refer to Steering Column Trim Covers Replacement.
3. Remove the instrument cluster trim panel. Refer to Instrument Cluster Trim Panel Replacement.
4. Lower the steering column.
5. Remove the instrument cluster (1) to I/P trim pad retaining screws (2).
6. Carefully remove the instrument cluster (1) from the instrument panel trim pad.
7. Disconnect the instrument cluster (1) electrical connector (2).

Important: When removing the instrument cluster, take care not scratch or damage the instrument cluster screen.

8. Remove the instrument cluster (1) from the I/P pad.

### Installation Procedure

1. Connect the electrical connector (2) to the Instrument cluster (1).

Important: When installing the instrument cluster, make sure the anti-rattle foam (1) is between the I/P trim pad and instrument cluster.

2. Install the instrument cluster into the I/P pad.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the instrument cluster (1) retaining screws (2).

Tighten
Tighten the screws (2) to 2 N·m (18 lb in).

4. Install the instrument panel (I/P) trim panel. Refer to Instrument Cluster Trim Panel Replacement.
5. Install the steering wheel upper trim cover. Refer to Steering Column Trim Covers Replacement.
6. Install the knee bolster. Refer to Knee Bolster Replacement.