For 1990-2009 cars

## Video Disc Player Display Bezel Replacement Display

### Removal Procedure

1. Remove the rear dome lamp assembly. Refer to Dome Lamp Replacement.
2. Remove the DVD screen surround to roof panel screw (1).

Important: Using a suitable tool disengage the retainers (3).

3. Remove the DVD screen surround (2) from the headlining trim (4).

### Installation Procedure

Important: Make sure all the retainers (3) engage the headlining trim (3).

1. Install the DVD screen surround (2) to the headlining trim (4).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the DVD screen surround to roof panel retaining screw (1).

Tighten
Tighten the screws to 1 N·m (18 lb in).

3. Install the rear dome lamp assembly. Refer to Dome Lamp Replacement.