For 1990-2009 cars

1. Install a NEW O-ring (2) on the oil level indicator tube (1).
2. Install the oil level indicator and tube (1) by sliding the oil level indicator and tube (1) down through the exhaust manifold (2).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the oil level indicator tube bracket to cylinder head retaining bolt (2).

Tighten
Tighten the bolt to 10 N·m (89 lb in).

4. Install the exhaust manifold heat shield (2).
5. Install the exhaust manifold heat shield to exhaust manifold retaining bolts (1).

Tighten
Tighten the bolts to 10 N·m (89 lb in).