For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement.
2. Remove the speaker. Refer to Radio Front Side Door Lower Speaker Replacement.
3. Detach the wiring harness to door retaining clip (1).

Important: Pull the water deflector (2) from the door (1) to release the adhesive bond.

4. Remove the water deflector (2) from the door (1).

### Installation Procedure

Important: Firmly press the water deflector (2) where adhesive is applied to make sure of a water tight seal to the door (1).

1. Install the water deflector (2) to the door (1).
2. Attach the wiring harness to door retaining clip (1).
3. Install the speaker. Refer to Front Side Door Trim Panel Replacement.
4. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement.