For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Rear Side Door Trim Panel Replacement.
2. Remove the speaker. Refer to Radio Rear Side Door Speaker Replacement.
3. Remove the water deflector. Refer to Rear Side Door Water Deflector Replacement.
4. Raise and support the window in the full up position.
5. Loosen the window regulator to window glass retaining bolts (1).
6. Support the window glass.
7. Lower the window regulator approximately 1/2 way down.
8. Disconnect the window regulator electrical connector (1).
9. Remove the window regulator to door retaining bolts (1).
10. Remove the window regulator (1) through the large access hole in the door (2).

### Installation Procedure

1. Position the window regulator (1) through the large access hole in the door (2).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the window regulator to door retaining bolts (1).

Tighten
Tighten the bolts to 10 N-m (89 lb in).

3. Remove the support from the window.
4. Lower the window into the window regulator clamps.
5. Connect the window regulator electrical connector (1).
6. Start the vehicle to make sure maximum power to the window motor. This is required to fully seat the window for adjustment.
7. Raise the window to the full up position.
8. Tighten the window regulator to window glass retaining bolts (1).

Tighten
Tighten the bolts to 8 N-m (70 lb in).

9. Inspect the window for correct operation and a tight seal.
10. Shut off the vehicle.
11. Install the water deflector. Refer to Rear Side Door Water Deflector Replacement.
12. Install the speaker. Refer to Radio Rear Side Door Speaker Replacement.
13. Install the door trim panel. Refer to Rear Side Door Trim Panel Replacement.