For 1990-2009 cars

## Windshield Wiper and Washer Switch Replacement LHD

### Removal Procedure

1. Remove the steering column trim covers. Refer to Steering Column Trim Covers Replacement.
2. Press top and bottom tabs in and Pull the wiper/washer switch out if the column assembly.
3. Disconnect the wiper/washer switch electrical connector.

### Installation Procedure

1. Install the Wipers/Washer signal switch to the steering column. Listen for an audible click to confirm fitting.
2. Connect the wiper/washer switch electrical connector.
3. Install the steering column trim covers. Refer to Steering Column Trim Covers Replacement.
4. Test wiper and washer system for correct operation.