For 1990-2009 cars

### Removal Procedure

1. Select park/1st gear position in the transmission and apply the park brake.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

Caution: Refer to Safety Glasses Caution in the Preface section.

2. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
3. Remove the intermediate exhaust assembly. Refer to Exhaust Crossover Pipe Replacement .
4. Remove the propeller shaft heat shield. Refer to Exhaust Heat Shield Replacement - Center .

Important: Observe the orientation of the rubber couplings with reference to the differential flange and the transmission flange. This will minimise the potential of incorrect propeller shaft installation.

5. Mark the rubber coupling (1) in relation to the differential flange (2).

Important: With the aid of an assistant or suitable jack support the propeller shaft (2).

6. Remove the rubber coupling to differential flange retaining bolts (1).

Important: Observe the orientation of the rubber couplings with reference to the differential flange and the transmission flange. This recommendation will minimise the potential of incorrect propeller shaft installation.

7. Mark the rubber coupling (2) in relation to the transmission flange (1).

Important: With the aid of an assistant or suitable jack support the propeller shaft.

Important: Torque prevailing nuts with are single use parts and must be discarded after removal.

8. Remove the rubber coupling to transmission flange retaining bolts (1) and torque prevailing nuts (2).

Discard the nuts.

Important: With the aid of an assistant or suitable jack support the propeller shaft (2).

9. Remove the centre bearing to body retaining bolts (1).
10. Disconnect the propeller shaft (2) from the differential flange.
11. Remove the propeller shaft (2) from the vehicle.
12. Inspect the propeller shaft (2) assembly for excessive wear and/or damage. Inspect the following:

• | Propeller shaft. For replacement refer to Propeller Shaft Replacement .

• | Rubber coupling. For replacement refer to Rear Propeller Shaft Coupling Replacement .

• | Centre bearing. For replacement refer to Propeller Shaft Center Support Bearing Replacement .

• | Universal joint. For replacement refer to Universal Joint Replacement .

### Installation Procedure

Important: Align the marks on the rubber coupling (1) to differential flange (2) made prior to removal.

1. Connect the rubber coupling (1) to the differential flange (2).

Notice: Refer to Fastener Notice in the Preface section.

Important: With the aid of an assistant or suitable jack support the propeller shaft (2) to the differential flange (3).

2. Install the rubber coupling to differential flange retaining bolts (1).

Tighten
Tighten the bolts to 115 N-m (85 lb ft).

Important: Align the marks on the rubber coupling (2) to transmission flange (1) made prior to removal.

3. Connect the rubber coupling (2) to transmission flange (1).

Important: With the aid of an assistant or suitable jack support the propeller shaft (2).

Important: The centre bearing to body retaining bolts (1) must not be fully tightened at this stage.

4. Install the centre bearing to body retaining bolts (1).

Important: With the aid of an assistant or suitable jack support the propeller shaft.

5. Install the rubber coupling to transmission flange bolts (1) and NEW torque prevailing nuts (2).

Tighten
Tighten the bolts and nuts to 100 N-m (72 lb ft).

6. Tighten the centre bearing to body retaining bolts (1).

Tighten
Tighten the bolts to 22 N-m (16 lb ft).

7. Install the propeller shaft heat shield. Refer to Exhaust Heat Shield Replacement - Center .
8. Install the intermediate exhaust assembly. Refer to Exhaust Crossover Pipe Replacement .
9. Remove the safety stands.
10. Lower the vehicle to the ground.