For 1990-2009 cars

## Front Fog Lamp Replacement LWB SWB

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the battery ground cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the air deflector from the front end of the vehicle. Refer to Front Air Deflector Replacement.
3. Disconnect the electrical connector (3) from the fog lamp assembly.
4. Remove the fasteners (1) that secure the front fog lamp assembly (2) to the front fascia.
5. Remove the front fog lamp assembly from the vehicle.

### Installation Procedure

Important: Do not handle the quartz envelope of the headlight bulb. Wipe the quartz envelope immediately with methylated spirits if it is touched accidentally or the performance of the bulb will deteriorate.

1. Install the front fog lamp assembly (2) to the front facia assembly.

Notice: Refer to Fastener Notice in the Preface section.

2. Install and tighten the retaining screws to secure the front fog lamp assembly to the front fascia.

Tighten
Tighten the retaining screws to 2.0 N·m (18 lb in).

3. Connect the electrical connector (3) to the fog lamp assembly.
4. Install the air deflector to the front end of the vehicle. Refer to Front Air Deflector Replacement.

Caution: Refer to Battery Disconnect Caution in the Preface section.

5. Connect the battery ground cable. Refer to Battery Negative Cable Disconnection and Connection.
6. Adjust the fog lamps. Refer to Fog Lamp Aiming.