For 1990-2009 cars

## Fastener Tightening Specifications Unit Repair

#### Fastener Tightening Specifications

Description of Usage | Ref No.* | Qty | Specification
--- | --- | --- | ---
Metric | English
Accumulator Housing to Valve Body | 318 | 12 | 11 N·m | 97 lb. in
Channel Plate to Valve Body | 300 | 7 | 11 N·m | 97 lb. in
Converter Housing to Case | 2 | 7 | 22 N·m | 16 lb. ft
Drain Plug to Fluid Pan | 63 | 1 | 20 N·m | 15 lb. ft
Extension Housing to Case | 35 | 7 | 22 N·m | 16 lb. ft
Fluid Pan to Case | 65 | 20 | 11 N·m | 97 lb. in
Front Control Valve Body to Top Channel Plate | 50 | 2 | 11 N·m | 97 lb. in
Input Speed Sensor to Case | 45 | 1 | 11 N·m | 97 lb. in
Output Speed Sensor to Case | 43 | 1 | 11 N·m | 97 lb. in
Parking Pawl Actuator Bracket to Case | 609 | 2 | 22 N·m | 16 lb. ft
Prop Shaft Flange to Output Shaft | 34 | 1 | 57 N·m | 42 lb. ft
Torque Converter Housing Seal Bolt | 228 | 2 | 3.6 N·m | 31.86 lb. in
Transmission Fluid Pump Cover to Torque Converter Housing | 240 | 6 | 11 N·m | 97 lb. in
Transmission Fluid Pump Cover to Torque Converter Housing | 241 | 5 | 22 N·m | 16 lb. ft
Transmission Level Hole Plug to Case | 36 | 1 | 20 N·m | 15 lb. ft
Transmission Pressure Test Plug to Case | 40 | 1 | 11 N·m | 97 lb. in
Valve Body to Case | 49 | 2 | 11 N·m | 97 lb. in
Valve Body to Case | 51 | 6 | 11 N·m | 97 lb. in
Valve Body to Case | 53 | 1 | 11 N·m | 97 lb. in
Valve Body to Channel Plate | 53 | 1 | 11 N·m | 97 lb. in
* Reference Number refers to the callout number on the disassembled view.

## Fastener Tightening Specifications On Vehicle

#### Fastener Tightening Specifications (On Vehicle)

Application | Specification
--- | ---
Metric | English
Case Extension Housing Retaining Bolt | 22 N·m | 16 lb. ft
Control Valve Body Assembly Retaining Bolt | 11 N·m | 97 lb. in
Detent Spring Retaining Bolt | 11 N·m | 97 lb. in
Drive Flange Retaining Nut | 60 N·m | 44 lb. ft
Fluid Cooler Pipe Brace Retaining Bolt | 50 N·m | 37 lb. ft
Fluid Cooler Pipe Retaining Bolt | 25 N·m | 18 lb. ft
Fluid Drain Retaining Plug | 20 N·m | 15 lb. ft
Fluid Fill Retaining Plug | 20 N·m | 15 lb. ft
Fluid Pan Retaining Bolt | 11 N·m | 97 lb. in
Input Speed Sensor Retaining Bolt | 11 N·m | 97 lb. in
Manual Shift Shaft Retaining Nut | 9 N·m | 80 lb. in
Oil Pressure Test Retaining Plug | 11 N·m | 97 lb. in
Output Speed Sensor Retaining Bolt | 11 N·m | 97 lb. in
Shift Control Assembly to Tunnel Reinforcement Retaining Nut | 12 N·m | 106 lb. in
Shift Control Linkage Adjustment Retaining Nut | 9 N·m | 80 lb. in
Torque Converter Retaining Bolt | 63 N·m | 46 lb. ft
Torque Converter Seal Retaining Bolt | 3.6 N·m | 31.9 lb. in
Transmission Mounting Retaining Bolt M10x1.5 | 50 N·m | 37 lb. ft
Transmission Mounting Retaining Bolt M12x1.75 | 75 N·m | 55 lb. ft
Front Sub Frame Bolts | 160 N·m | 118 lb. ft
Transmission Support to Underbody Retaining Bolt | 63 N·m | 46 lb. ft