For 1990-2009 cars

### Removal Procedure

1. Using a suitable tool disengage the trim panel (1) retaining clips.
2. Remove the trim panel (1) from the I/P pad.
3. If required, repeat for opposite side

### Installation Procedure

1. Align the trim panel (1) with the I/P pad.
2. Install the trim panel (1) to the I/P pad by engaging the retaining clips.
3. Ensure the trim panel (1) is flush with the I/P pad.
4. If required, repeat for opposite side