For 1990-2009 cars

### Diagnostic Instructions

• | Perform the Diagnostic System Check - Vehicle prior to using this diagnostic procedure.

• | Review Strategy Based Diagnosis for an overview of the diagnostic approach.

• | Diagnostic Procedure Instructions provides an overview of each diagnostic category.

### DTC Descriptor

DTC B1335 03: Screen 1 Power Supply Voltage Below Threshold
DTC B1335 07: Screen 1 Power Supply Voltage Above Threshold
DTC B1340 03: Screen 2 Power Supply Voltage Below Threshold
DTC B1340 07: Screen 2 Power Supply Voltage Above Threshold

### Circuit/System Description

With the ignition in either the ACC or ON positions, the DVD screens each receive an individual 12V power supply. The DVD screen power supply is distributed via the Audio/Video Interface Module. DTCs B1335 03 and B1335 07 relate to the headlining DVD screen installed to lower level vehicles and the right front head restraint DVD screen on higher level vehicles. DTCs B1340 03 and B1340 07 relate to the left front head restraint DVD screen on higher level vehicles.

### Conditions for Running DTC

#### B1335 03, B1340 03

DTC B1335 03 or B1340 03 will set to indicate the B+ positive supplied to the DVD screen is below the threshold.

#### B1335 07, B1340 07

DTC B1335 07 or B1340 07 will set to indicate the B+ positive supplied to the DVD screen is above the threshold.

### Conditions for Setting the DTCs

These DTCs run continuously once the following condition is met:

The supplied power to the DVD screen is between 9 - 16V.

### Action Taken When the DTC Sets

When DTC B1335 or B1340 is set, the DVD screen will not turn ON.

### Conditions for Clearing the DTC

• | The condition for setting the DTC is no longer present.

• | The history DTC will clear after 50 fault-free ignition cycles.

### Reference Information

#### Schematic Reference

Video System Schematics

#### Connector End View Reference

Component Connector End Views

#### Description and Operation

Video Entertainment System Description and Operation

#### Electrical Information Reference

• | Circuit Testing

• | Connector Repairs

• | Testing for Intermittent Conditions and Poor Connections

• | Wiring Repairs

#### Scan Tool Reference

Control Module References for scan tool information

### Diagnostic Aids

The DVD screen power supply is distributed via the rear seat entertainment interface module. DTC B1335 03 or DTC B1340 03 could set concurrently with DTC B1423 03 as a result of the B+ positive supplied to the Audio/Video Interface Module being below the threshold. DTC B1335 07 or DTC B1340 07 could set concurrently with DTC B1423 07 as a result of the B+ positive supplied to the Audio/Video Interface Module being above the threshold. In the event of these DTCs setting together either DTC B1423 03 or DTC B1423 07 should be diagnosed first. If either DTC B1423 03 or DTC B1423 07 is not set it would suggest that the fault exists after the Audio/Video Interface Module and is within the B+ positive supply to the DVD screen or a fault within the component.

### Circuit/System Testing

1. Ignition OFF, disconnect the DVD screen harness connector.
2. Ignition OFF, test for less than 3 Ω between the ground circuit at the rear seat entertainment interface module harness connector and a ground.

⇒ | If greater than the specified range, test the circuti for an open/high resistance.

3. Ignition ON, test for B+ between the battery positive voltage circuit at the DVD screen harness connector and ground.

⇒ | If not within specified range, test the battery positive voltage circuit for an open/high resistance. If the circuit tests normal replace the Audio/Video Interface Module.

4. If all circuits test normal, replace the DVD screen.

### Repair Instructions

Perform the Diagnostic Repair Verification after completing the diagnostic procedure.

• | Video Display Replacement

• | Audio/Video Interface Module Replacement