For 1990-2009 cars

## Blower Motor Replacement LHD

### Removal Procedure

1. Remove the right closeout insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Right Side .
2. Remove the instrument panel (I/P) compartment. Refer to Instrument Panel Compartment Replacement .
3. Disconnect the blower motor electrical connector.
4. Disconnect the blower motor processor electrical connector.
5. Remove the blower motor retaining screws (1).
6. Remove the blower motor.

### Installation Procedure

1. Install the blower motor.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the blower motor retaining screws (1).

Tighten
Tighten the screws to 1.5 N·m (13 lb in).

3. Connect the blower motor processor electrical connector.
4. Connect the blower motor electrical connector.
5. Install the I/P compartment. Refer to Instrument Panel Compartment Replacement .
6. Install the right closeout insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Right Side .