For 1990-2009 cars

### Removal Procedure

1. Remove the air cleaner intake duct. Refer to Air Cleaner Inlet Duct Replacement .
2. Remove air cleaner element refer to Air Cleaner Element Replacement
3. Remove the air cleaner to chassis retaining bolts (1).
4. Remove the air cleaner assembly from the vehicle.

### Installation Procedure

1. Install the air cleaner to the vehicle.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the air cleaner to chassis retaining bolts (1).

Tighten
Tighten the air cleaner to chassis bolts to 9 N·m (78 lb in).

3. Install the air cleaner element Refer to Air Cleaner Element Replacement
4. Install the air cleaner intake duct. Refer to Air Cleaner Inlet Duct Replacement .