For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Rear Side Door Trim Panel Replacement.
2. Remove the speaker. Refer to Radio Rear Side Door Speaker Replacement in Entertainment.
3. Remove the water deflector. Refer to Rear Side Door Water Deflector Replacement.
4. Remove the window regulator. Refer to Rear Side Door Window Regulator Replacement.
5. Remove the window regulator motor to window regulator retaining bolts (1).
6. Remove the window regulator motor (1) from the window regulator (2).

### Installation Procedure

1. Position the window regulator motor (1) to the window regulator (2).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the window regulator motor to window regulator retaining bolts (1).

Tighten
Tighten the bolts to 8 N-m (71 lb in).

3. Install the window regulator. Refer to Rear Side Door Window Regulator Replacement.
4. Install the water deflector. Refer to Rear Side Door Water Deflector Replacement.
5. Install the speaker. Refer to Radio Rear Side Door Speaker Replacement in Entertainment.
6. Install the door trim panel. Refer to Rear Side Door Trim Panel Replacement.