For 1990-2009 cars

## Instrument Panel Storage Compartment Replacement LWB

### Removal Procedure

1. Remove the trim plate. Refer to Console Trim Plate Replacement.
2. Remove the storage compartment (1) to I/P tower retaining screws (2).
3. Remove the storage compartment (1) from the I/P tower.

### Installation Procedure

1. Install the storage compartment (1) to the I/P tower.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the storage compartment to I/P tower retaining screws (2).

Tighten
Tighten the screws (2) to 2 N·m (18 lb in).

3. Install the trim plate. Refer to Console Trim Plate Replacement.
4. Operate the storage compartment lid for correct operation.