For 1990-2009 cars

Checks | Causes
--- | ---
Centre (with 2-6 Low and Reverse Clutch) Support Assembly (67) |

• | Inspect for a damaged centre support assembly (459).

• | Inspect for worn or damaged output carrier outer sun gear shaft front and rear bushing (458 and 460).

Centre Support Retaining Ring (66) | Inspect for damage.
Output Carrier Assembly (68) | Inspect for a worn or damaged centre support roller bearing assembly (485).
2-6 and 3-5-R Clutch Hub Thrust Bearing Assembly (65) | Inspect the bearing for wear or damage.