For 1990-2009 cars

### Removal Procedure

Important: If the roof weld joint reveal moulding cracks, breaks or is damaged in any way, replace the moulding.

Important: Take care not to damage the paint on the vehicle when prying the roof weld joint reveal moulding from the roof.

1. Starting at the windshield pillar rear, carefully pry off the roof weld joint reveal moulding from the roof weld joint, taking care not to break the roof weld joint reveal moulding retaining clips (2).
2. Remove the roof weld joint reveal moulding (1).
3. Clean the accessible roof weld joint with a suitable cleaning solution, using a lint free cloth.

### Installation Procedure

Important: Make sure that the rear datum pin is positioned correctly.

1. Position the roof weld joint reveal moulding on the vehicle and slide the rear end of the moulding into the rear moulding retainer.
2. Seat the roof weld joint reveal moulding in the roof weld joint and starting at the rear, carefully engage the roof weld joint reveal moulding retaining clips (2) into position.