For 1990-2009 cars

### Removal Procedure

Important: The front floor console front cover (1) is retained by clips.

1. Grasp the front floor console front cover (1) at (a) and pull upwards to disengage the retaining clips from the floor console (2).
2. Disconnect the window and exterior mirror switch electrical connector (2).
3. Disconnect the Traction Control/ESP, Power and Puddle lamp switch (if fitted) assembly electrical connector (3).
4. Remove the front floor console front cover (1).

Important: Remove the power window/mirror switch (2) by releasing from the retaining clips (3) on the front floor console cover (1).

5. Remove the power window/mirror switch (2) from the front floor console front cover (1).

### Installation Procedure

Important: Install the power window/mirror switch (2) by attaching to the retaining clips (3) on the front floor console cover (1).

1. Install the power window/mirror switch (2) to the front floor console front cover (1).
2. Position the front floor console front cover (1).
3. Connect the window and exterior mirror switch electrical connector (2).
4. Connect the Traction Control/ESP, Power and Puddle lamp switch (if fitted) assembly electrical connector (3).

Important: The front floor console front cover (1) is retained by clips.

5. Install the front floor console front cover (1) and push downwards at (a) to engage the retaining clips to the floor console (2).