For 1990-2009 cars

## Mode Valve Actuator Replacement LHD

### Removal Procedure

1. Remove the instrument panel (I/P) carrier. Refer to Instrument Panel Retainer Replacement .
2. Disconnect the mode actuator electrical connector (1).
3. Remove the mode actuator (2) to HVAC unit retaining screws (1).
4. Remove the mode actuator (2) from the HVAC unit.

### Installation Procedure

1. Install the mode actuator (1) to the HVAC unit.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the retaining screws (1) to mode actuator (2)..

Tighten
Tighten the screws to 1 N·m (9 lb in).

3. Connect the electrical connector (1) to the mode actuator.
4. Install the I/P carrier. Refer to Instrument Panel Retainer Replacement .