Technical Service Bulletins GMC Truck Caballero 1986

For 1990-2009 cars

# Technical Service Bulletins

- 2008-06-04: No Movement When Transmission is Shifted to Drive or Third - Normal Operation When Shifted to Second, First or Reverse (Replace Forward Sprag Assembly) (08-07-30-027)
- 2008-04-04: 4L60 Automatic Transmission - New Sprag Assembly, Forward Clutch to Overrun Clutch Hub (08-07-30-017)
- 2007-12-05: 60 Degree V6 Engine Oil Leak at Crankshaft Front Oil Seal (Use New Crankshaft Front Oil Seal Installer Tool EN-48869) (07-06-01-023)
- 2006-01-27: Service VME - Use Correct Engine Oil Drain Plug - keywords drain engine leak oil pan plug replace (PIP3696)
- 2006-01-18: Info - New Product Feedback Form and Process for Automatic Transmission Core Returns (01-07-30-029A)
- 2004-03-18: No TCC Apply , MIL On , TCC Surge , Possible P0740 , P1870 , or 39 after Installation of Reman ( SRTA ) 4T60 / 4T60E - kw case cover converter slip transmission (PI01880A)
- 2001-04-06: Info - Current CIPS Campaign Number to Previous DIvisional Campaign Number (01-00-89-008)
- 2000-09-28: High Oil Consumption After Installation of Goodwrench Remanufactured Engine (00-06-01-019)
- 1999-12-23: Info - Dealer Installed Rear Seat Lap/Shoulder Belt Kits (99-09-40-006)
- 1997-12-11: WARRANTY ADMIN - ACDELCO REMANUFACTURED ENGINES (72-05-07)
- 1997-01-01: GUIDELINES FOR RETROFITTING R-12 VEH. TO R-134A (43-12-07E)
- 1996-12-01: SERVICE ADMINISTRATION - WARRANTY CLAIMS PROCESSING (31-05-03C)
- 1996-05-01: AC DELCO LOCATOR SVCS FOR DELCO ELECTRONICS EXCHANGE (58-83-02B)
- 1995-10-10: WARRANTY INFORMATION ALL MODELS - ALL YEARS (58-05-03)
- 1995-08-10: REVISED TECH 1 MASS STORAGE CARTRIDGE (MSC) OXYGEN SENSOR (51-65-47)
- 1995-07-19: WARRANTY ADMINISTRATION - INFO. ON PREVIOUSLY RELEASED (56-05-03)
- 1995-06-12: INFO. ON REFORMULATED GASOLINE (RFG) (57-01-02)
- 1995-06-01: CAMPAIGN: SERVICE PART FUEL TANK SENDER RING WELDS (91-C-51)
- 1995-05-15: INFORMATION ON CONTAMINATED R12 REFRIGERANT TESTING (53-12-05)
- 1995-04-27: INFORMATION ON GM CAMPAIGN IDENTIFICATION LABEL (51-01-03)
- 1995-04-01: INFORMATION ON SIERRA-BRAND ENGINE COOLANT (43-62-01B)
- 1995-03-28: WARRANTY ADMINISTRATION DEALER/RETAILER ADMINISTRATION (57-05-01)
- 1995-03-01: SMU - SECTION 0 - GENERAL INFORMATION (57-02-01)
- 1995-02-03: SMU - INFO. ON INSPECTION/ MAINTENANCE (I/M) EMISSIONS (51-65-02)
- 1995-01-11: ENHANCED EMISSION INSPECTION MAINTENANCE PROGRAM (43-65-10)
- 1994-11-29: INFO. ON ENHANCED EMISSION INSPECTION MAINTENANCE PROGRAM (43-65-07)
- 1994-10-25: REV. TO ADHESIVE CAULKING KIT, NEW PRIMERS & PART NUMBERS (43-10-48)
- 1994-09-15: DLR. PRODUCT CAMPAIGN BULLETIN NUMBERING SYSTEM (41-01-03)
- 1994-09-12: INFO. ON NEW PROM/MEMCAL IDENTIFICATION MARKINGS (44-65-01)
- 1994-09-08: CONTAMINATED A/C REFRIGERANT (INFORMATIONAL) (43-12-23)
- 1994-09-01: INFORMATION ANNOUNCING THE NEW CORPORATE BULLETIN (33-01-05A)
- 1994-08-16: OBTAINING TECHNICAL ASSISTANCE (I/M 240 REPAIRS) (43-65-06)
- 1994-07-18: INFORMATION ON RELEASE OF SERVICE PKG. FOR NICKEL TAPE (14-93-01)
- 1994-06-30: INFORMATION ON J39400 A/C LEAK DETECTOR MAINTENANCE KIT (43-12-18A)
- 1994-06-08: WARRANTY ADMINISTRATION - NEW LABOR OPERATION NUMBER (42-05-06)
- 1994-05-13: WARRANTY ADMINISTRATION - EMISSION WARR. PARTS COVERAGE (47-05-01)
- 1994-04-08: REDUCED PWR STEERING ASSIST AT LOW AMBIENT TEMPERATURES (03-32-06)
- 1994-03-29: ENHANCED INSPECTION MAINTENANCE PROGRAMS (43-65-05)
- 1994-02-01: INFORMATION ON AFTER MARKET ANTI-LOCK BRAKE SYS. PRODUCTS (43-50-01)
- 1993-12-22: RETROFITTING R-12 VEHICLES TO R-134A (INFORMATIONAL) (33-12-26)
- 1993-06-01: INFORMATION ON COSMETIC DAMAGE TO ALUMINUM WHEELS DURING BAL. (93-3E-67)
- 1993-05-25: RECYCLING OF USED OIL FILTERS (INFORMATIONAL) (93-0A-90)
- 1993-05-19: INFO. ON SERVICING VEHICLE WITH CONTAMINATED TRANS. FLUID (93-7A-84)
- 1993-05-19: INFO. ON SERVICING VEHICLE WITH CONTAMINATED TRANS. FLUID (93-7A-142)
- 1993-05-06: A/C R-134A REFRIGERANT (INFORMATION) (93-1B-78)
- 1993-05-06: A/C R-134A REFRIGERANT (INFORMATION) (93-1B-126)
- 1993-04-30: BINDING/STICKING LOCK CYLINDER RECOMMENDED LUBRICATIONS (93-10-194)
- 1993-03-16: ILLUSTRATED STEERING SYSTEM BLEED PROCEDURE (38-30-01A)
- 1993-03-01: DOOR LOCK CYLINDER RECOMMENDED LUBRICATIONS (93-10A1-52)
- 1993-01-27: INFO. ON FACTORS THAT AFFECT FUEL ECONOMY (30-65-02)
- 1992-12-01: ENG. MISS, HESITATION & ROUGH PIERCED SECONDARY IGNITION (93-6D-102)
- 1992-11-30: ALTERNATE REFRIGERANTS INFORMATION (93-1B-102)
- 1992-11-01: INDUSTRIAL FALLOUT-PAINT DAM. FINESSE TYPE REPAIRS (93-10-30)
- 1992-11-01: INDUSTRIAL FALLOUT-PAINT DAM. FINESSE TYPE REPAIRS (92-2-128)
- 1992-11-01: INDUSTRIAL FALLOUT-PAINT DAM. FINESSE TYPE REPAIRS (93-10-148)
- 1992-10-31: A/C COMPRESSOR SHAFT NUT REMOVAL (IMPROVED QUALITY) (93-1D-100)
- 1992-09-01: INFO. ON GMC TRUCK BULLETINS NEW NUMBERING SYSTEM (93-0A-01)
- 1992-09-01: ALTERNATE REFRIGERANTS INFORMATION (93-1B-8)
- 1992-06-22: PAINT CHIPS - EXTERIOR LEADING EDGES (APPLY CHIP PROTECTOR) (92-10-104)
- 1992-06-16: SERVICE GUILD: INFO ON AVOID DAMAGE TO TIRE WHEELS (92-3E-108)
- 1992-06-16: SERVICE GUILD: INFO ON AVOID DAMAGE TO TIRE WHEELS (92-3-123)
- 1992-05-31: BRAKE PULSATION SERVICE INFORMATION (88-5-121)
- 1992-05-27: A/C LEAK (DIAGNOSIS BULLETIN) ALL MODELS 1992 AND PRIOR (92-1B-92)
- 1992-04-30: ENGINE BLOCK HEATER LEAKS REPLACE HEATER WITH NEW P/N (92-6B-71A)
- 1992-04-03: ENG. BLOCK HEATER LEAK-INSTALL REDESIGNED BLOCK HEATER (92-6-116)
- 1992-04-01: PROM I.D. NOT RECOGNIZED BY THE T-100 (GM CAMS) TERMINAL (23-65-08)
- 1992-03-24: INFO ON COATED WHEEL WEIGHTS USED FOR ALUMINUM WHEELS (92-3E-74)
- 1992-03-24: INFO ON COATED WHEEL WEIGHTS USED FOR ALUMINUM WHEELS (92-3-121)
- 1991-11-07: INTERMIT TRANS DOWNSHIFT/SLIP DIAGNOSIS (92-7A-33)
- 1991-11-07: INTERMIT TRANS DOWNSHIFT/SLIP DIAGNOSIS (92-73L80-100)
- 1991-11-06: BINDING/STICKING LOCK CYLINDER RECOMMENDED LUBRICATIONS (92-2-141)
- 1991-10-15: A/C COMPRESSOR SHAFT NUT REMOVAL (IMPROVED QUALITY) (93-1B-11)
- 1991-10-02: DEXRON IIE A/T FLUID PREFERRED (GENERAL INFORMATION) (92-7A-19)
- 1991-10-02: DEXRON IIE A/T FLUID PREFERRED (GENERAL INFORMATION) (92-7-100)
- 1991-09-30: 3-4 CLUTCH/2-4 BAND SERVICE INFORMATION/SERVICE PROCEDURES (91-7-113)
- 1991-09-20: A/C REFRIGERANT LOSS DUE TO LOOSE OR MISSING ACCESS CAPS (91-1B-112A)
- 1991-08-15: LOCKING DIFFERENTIAL LUBRICANT (SERVICE INFORMATION) (91-4-109)
- 1991-08-14: SERVICE GUILD: COOLANT RECYCLING UPDATE (91-0-106)
- 1991-08-09: SERVICE GUILD: DETECTING ELECT INTERMITTENTS DIAGNOSTIC (92-8A-09)
- 1991-08-09: SERVICE GUILD: DETECTING ELECT INTERMITTENTS DIAGNOSTIC (92-8-102)
- 1991-08-08: SERVICE GUILD: EVALUATING PEENED SPACER PLATE (91-7A-141)
- 1991-08-08: SERVICE GUILD: EVALUATING PEENED SPACER PLATE (91-7-115)
- 1991-07-31: LOCKING REAR AXLE CHATTER (MAINT./WARRANTY INFO.) (91-4B-124)
- 1991-07-26: AC DELCO ADVANCE EXCHANGE PROGRAMS (REVIEW) (91-0A-131)
- 1991-07-24: DAMAGED ECM/PCM MIS-DIAGNOSIS INCORRECT 'TAP-TESTING' (91-6D-132)
- 1991-07-24: DAMAGED ECM/PCM MIS-DIAGNOSIS INCORRECT 'TAP-TESTING' (91-6-121)
- 1991-06-11: INFORMATION ON STATE EMISSION TESTING FOR ALL MODELS (91-6E-114)
- 1991-06-11: INFORMATION ON STATE EMISSION TESTING FOR ALL MODELS (91-6-120)
- 1991-05-23: INFO ON NON-FACTORY INSTALLED HYDRAULIC PARKING BRAKE (91-5-101)
- 1991-05-23: INFO ON NON-FACTORY INSTALLED HYDRAULIC PARKING BRAKE (91-5-140)
- 1991-05-15: BINDING OR INOP REVERSE STUCK 3-4 SEQ. VALVE 2-3 SHIFT (91-74L60-104)
- 1991-05-10: SERVICE GUILD: HIGH VOL.-LOW PRESSURE PAINT APPLICATION (91-10-109)
- 1991-05-10: SERVICE GUILD: HIGH VOL.-LOW PRESSURE PAINT APPLICATION (91-2-206)
- 1991-04-30: A/C REFRIGERANT LOSS DUE TO LOOSE/MISS. ACCESS FITTING CAP (91-1-123)
- 1991-04-22: BINDING OR INOP IN REVERSE STUCK 4-3 SEQUENCE VALVE (91-7A-87)
- 1991-04-19: DAMAGE TO ECM/PCM CIRCUIT BOARD WHEN INSTALLING MEM-CAL (91-6D-113)
- 1991-04-19: DAMAGE TO ECM/PCM CIRCUIT BOARD WHEN INSTALLING MEM-CAL (91-6-117)
- 1991-03-12: CHECKING CLEAR COAT THICKNESS BEFORE & AFTER PAINT FINESSE (91-10-82)
- 1991-03-12: PAINT ETCHING/STAINING AND PERMANENT WATER SPOTTING (91-10-83)
- 1991-03-12: PAINT ETCHING/STAINING AND PERMANENT WATER SPOTTING (91-2-175)
- 1991-03-12: CHECKING CLEAR COAT THICKNESS BEFORE & AFTER PAINT FINESSE (91-2-181)
- 1991-02-15: NO START/VEHICLE BATTERY DEAD PARASITIC CURRENT DRAIN TEST (91-6D-88)
- 1991-02-15: NO START/VEHICLE BATTERY DEAD PARASITIC CURRENT DRAIN TEST (91-8-172)
- 1990-12-31: CHATTERING WIPER BLADES OR WIPEABILITY (91-8D-39)
- 1990-12-31: CHATTERING WIPER BLADES OR WIPEABILITY (91-2-123)
- 1990-12-10: ELECTRO-MECHANICAL INSTRUMENT CLUSTER REPLACEMENT INFO (91-8C-47)
- 1990-09-21: CHECKING CONNECTOR TERMINAL CONTACT - METRI - PACK (91-8A-28)
- 1990-09-21: CHECKING CONNECTOR TERMINAL CONTACT - METRI - PACK (91-8-108)
- 1990-08-15: ENG. NO START AFTER EXTENDED STORAGE (VITON HOSE KIT) (90-6C-89)
- 1990-08-15: STATE EMISSIONS TESTING INFORMATION / PROCEDURE (91-6E-15)
- 1990-08-15: ENG. NO START AFTER EXTENDED STORAGE (VITON HOSE KIT) (90-6-113)
- 1990-04-26: SRTA PROGRAM INTRODUCTION PROCESSING PROCEDURE OUTLINED (87-7A-122)
- 1990-04-26: SRTA PROGRAM INTRODUCTION PROCESSING PROCEDURE OUTLINED (90-72004R-101)
- 1990-04-11: INSTALLATION GUIDELINES FOR AFTERMARKET ACCESSORIES (90-9-66)
- 1990-04-11: INSTALLATION GUIDELINES FOR AFTERMARKET ACCESSORIES (90-8-184)
- 1990-03-21: PARASITIC DRAIN ON BATTERY AMMETER CONNECTING PROCEDURE (91-6D-03)
- 1990-03-21: PARASITIC DRAIN ON BATTERY AMMETER CONNECTING PROCEDURE (90-8-170)
- 1990-01-04: LOCKING DIFFERENTIAL (G80) LUBRICANT SERVICE INFORMATION (90-4-103)
- 1989-11-14: NEW VIP OVERNIGHT SERVICE PARTS DELIVERY PROGRAM (90-0A-18)
- 1989-11-09: LOOSE CARPET ON SIDE WALL TRIM PADS (REPAIR PROCEDURE) (90-10-21)
- 1989-11-09: LOOSE CARPET ON SIDE WALL TRIM PADS (REPAIR PROCEDURE) (90-2-114)
- 1989-10-06: TIRE COMPANY WARRANTY ASSISTANCE PROGRAMS (92-3E-37)
- 1989-10-03: A/C ODOR ON TRUCKS (CLEANING PROCEDURE) (89-1B-111)
- 1989-09-27: SERVICE GUILD: USE OF FUEL WITH 15% MTBE IN ALL GM VEH. (89-0A-119)
- 1989-09-21: GMC. TRUCK SERVICE BULLETINS NUMBERING SYS. GROUP CODE INFO (90-0A-08)
- 1989-09-18: PACKARD 32 WAY CONNECTOR IDENTIFICATION APPLICATIONS (89-8-206)
- 1989-08-18: SERVICE GUILD: RECONSTITUTED ANTI-FREEZE INFORMATION (90-0A-39)
- 1989-08-18: SERVICE GUILD: RECONSTITUTED ANTI-FREEZE INFORMATION (90-0-101)
- 1989-08-10: CFC REDUCTION AND REFRIGERANT RECOVERY (RECYCLING PROGRAM) (90-0A-22)
- 1989-08-10: CFC REDUCTION AND REFRIGERANT RECOVERY (RECYCLING PROGRAM) (89-1-126)
- 1989-05-31: EVALUATING DRIVELINE VIBRATION (DIAGNOSIS FAULT TREE) (89-T-73)
- 1989-05-31: EVALUATING DRIVELINE VIBRATION (DIAGNOSIS FAULT TREE) (89-0-116)
- 1989-04-16: MOAN NOISE WITH A/C ON INSTALL NEW COMPRESSOR PULLEY (88-T-209)
- 1989-04-16: MOAN NOISE WITH A/C ON INSTALL NEW COMPRESSOR PULLEY (88-1-120)
- 1989-03-31: LIGHT BRAKE DRAG-may BE BRAKE SWITCH ADJUSTMENT (89-T-65)
- 1989-03-31: LIGHT BRAKE DRAG-may BE BRAKE SWITCH ADJUSTMENT (89-5-116)
- 1989-03-21: BRAKE BOOSTER PUSH ROD HEIGHT GAGE (REVISED GAGE) (89-T-51)
- 1989-03-21: BRAKE BOOSTER PUSH ROD HEIGHT GAGE (REVISED GAGE) (89-5-115)
- 1989-02-15: NO ENGINE BRAKING IN DRIVE NEW PISTON-FRONT ACCUMULATOR (88-T-200)
- 1989-02-15: NO ENGINE BRAKING IN DRIVE NEW PISTON-FRONT ACCUMULATOR (897400-100)
- 1989-02-09: A/C REFRIGERANT LOSS DUE TO LOOSE/ MISSING ACCESS FIT. CAP (89-T-78)
- 1989-02-09: A/C REFRIGERANT LOSS DUE TO LOOSE/ MISSING ACCESS FIT. CAP (89-1-112)
- 1989-02-03: THM 400/475 PRODUCT UPDATE BOOK (89-7400-104)
- 1989-01-10: CAST ALUMINUM WHEEL POROSITY (REPAIR PROC. & SEALER) (89-3-105)
- 1988-12-26: SERVICE GUILD: FUEL PUMP STRAINER IN-TANK FILTER/SOCK (89-T-36)
- 1988-12-26: SERVICE GUILD: FUEL PUMP STRAINER IN-TANK FILTER/SOCK (88-6-125)
- 1988-10-03: ENGINE OIL REQUIREMENTS/INFO (ALL MD WITH TURBO) (88-T-159)
- 1988-10-03: ENGINE OIL REQUIREMENTS/INFO (ALL MD WITH TURBO) (88-6-506)
- 1988-08-08: ELECTROSTATIC DISCHARGE DAMAGE TO ECM (INFO. TO PREVENT) (88-8-168)
- 1988-07-18: SERVICE REPLACEMENT TRANSMISSION ASSEMBLY UPDATE (88-7-108)
- 1988-06-20: HOOD SHEET METAL MOVEMENT/ VIBRATION(NEW ADHESIVE AVAIL.) (88-T-130)
- 1988-06-20: HOOD SHEET METAL MOVEMENT/ VIBRATION(NEW ADHESIVE AVAIL.) (88-2-195)
- 1988-02-29: ENG. MISS,HESITATION & ROUGH PIERCED SEC. IGN. COMPONENTS (88-6-106)
- 1988-02-22: ERRATIC OR NO UPSHIFT NEW GOVERNOR DRIVEN GEAR (88-T-99)
- 1988-02-22: ERRATIC OR NO UPSHIFT NEW GOVERNOR DRIVEN GEAR (88-7400-101)
- 1988-02-01: ENG. MISS, HESITATION & ROUGH PIERCED SEC. IGN. COMPONENTS (88-T-17)
- 1987-12-01: R-22 REFRIGERANT ALL TRUCK MODELS (88-T-65)
- 1987-12-01: DAMAGE TO WIRING TERMINALS ON ENGINE SENSORS-METRI-PACK 150 (88-T-76)
- 1987-12-01: DAMAGE TO WIRING TERMINALS ON ENGINE SENSORS-METRI-PACK 150 (88-8-117)
- 1987-11-16: TIRE WARRANTIES IRREGULAR/PREMATURE WEAR (88-T-66)
- 1987-11-16: TIRE WARRANTIES IRREGULAR/PREMATURE WEAR (88-3-104)
- 1987-10-19: INSTRUMENT CLUSTER EXCHANGE PROGRAM INFORMATION (88-8-106)
- 1987-09-04: ECM RESET/ FAILURE DIAGNOSIS INFORMATION (87-6-117)
- 1987-07-31: TRAILER BRAKES INFORMATION (88-T-27)
- 1987-07-31: TRAILER BRAKES INFORMATION (88-5-100)
- 1987-06-19: NEW SECOND SERVO APPLY PIN 700R4- SEAL ELIMINATION (88-T-44)
- 1987-06-19: NEW SECOND SERVO APPLY PIN 700R4- SEAL ELIMINATION (87-7700-108)
- 1987-06-03: TIRE COMPANY ASSISTANCE PROGRAM (88-T-19)
- 1987-05-14: NEW ECM TEST PROCEDURES ALL ECM EQUIPPED VEHICLES (87-T-57)
- 1987-05-14: NEW ECM TEST PROCEDURES ALL ECM EQUIPPED VEHICLES (87-6-115)
- 1987-05-14: WARM/HOT HESITATION FUEL VAPOR CONTROL KIT (P/N) (86-T-148)
- 1987-05-14: WARM/HOT HESITATION FUEL VAPOR CONTROL KIT (P/N) (86-650-113)
- 1987-04-10: OIL CONTAMINATED BY GAS OIL CHANGE REQUIREMENTS (87-T-50)
- 1987-04-07: SURGE AFTER TCC ENGAGEMENT NEW PROM P/N'S LISTED (86-T-146)
- 1987-04-07: SURGE AFTER TCC ENGAGEMENT NEW PROM P/N'S LISTED (86-650-111)
- 1986-12-15: INSTRUMENT CLUSTER EXCHANGE PROGRAM INFORMATION (87-8-113)
- 1986-12-04: ENGINE SURGE AFTER HOT SOAK CARB. PRIMARY METERING JETS (86-B-80)
- 1986-11-07: VIBRATION DIAGNOSIS 'REED' TACHOMETER INFORMATION (87-T-9)
- 1986-11-06: OIL LEAK AT OIL PAN DRAIN PLUG V-8, V6, OHV L4 CARS & TRUCKS (86-B-119)
- 1986-11-06: OIL LEAK AT OIL PAN DRAIN PLUG V-8, V6, OHV L4 CARS & TRUCKS (86-6-122)
- 1986-10-20: USE OF UNLEADED GASOLINE IN VEHICLES USING LEADED GAS (87-6-100)
- 1986-09-29: TIMING CHAIN COVER OIL LEAK R AND R PROCEDURE CHANGE (86-650-105)
- 1986-09-24: CHATTERING WIPER BLADES CLEAN BLADES/GLASS (84-B-65)
- 1986-09-24: REVISED:CHATTERING BLADES CLEAN BLADES/GLASS (84-2-140)
- 1986-09-24: CHATTERING WIPER BLADES CLEAN BLADES/GLASS (87-2-106)
- 1986-09-23: USE OF UNLEADED GASOLINE VEHICLES USING LEADED GAS (87-0-104)
- 1986-09-15: PAINT/CARE OF CAR FINISHES ALL VEHICLES AFFECTED (87-2-100)
- 1986-09-04: A/T OIL COOLER FLUSHING ALL THM A/T MODELS (87-T-5)
- 1986-09-04: A/T OIL COOLER FLUSHING ALL THM A/T MODELS (87-7-100)
- 1986-08-28: COLOR SANDING NOT RECOMMENDED BASECOAT/CLEARCOAT VEHICLES (87-T-2)
- 1986-08-28: SQUEAK NOISE IN STEERING WHEEL LUBRICATE TILT WHEEL ASSEMBLY (87-T-3)
- 1986-08-28: SERVICE GUILD: ELECTROSTATIC DISCHARGE DAMAGE (87-T-4)
- 1986-08-28: SQUEAK NOISE IN STEERING WHEEL LUBRICATE TILT WHEEL ASSEMBLY (87-3-100)
- 1986-08-28: SERVICE GUILD: ELECTROSTATIC DISCHARGE DAMAGE (87-8-102)
- 1986-07-15: 5MT STARTER MOTOR CLICKS FAILS TO ENGAGE RING GEAR (86-B-112)
- 1986-07-15: TRANSMISSION BULLETIN SUMMARY LISTING (86-B-78)
- 1986-07-15: 5MT STARTER MOTOR CLICKS FAILS TO ENGAGE RING GEAR (86-6-124)
- 1986-07-15: TRANSMISSION BULLETIN SUMMARY LISTING (86-7-105)
- 1986-06-20: CLEAR COAT ON ALUMINUM WHEELS REPAIR PROCEDURE OUTLINED (86-B-98)
- 1986-06-20: CLEAN, PAINT & COATING OF ALUMINUM WHEELS (85-3-118)
- 1986-05-19: ENGINE SURGE AFTER HOT SOAK CARB. PRIMARY METERING JETS (86-650-102)
- 1986-05-12: SERVICE MANUAL SUPPLEMENT REVISED CARBURETOR NUMBERS (86-6-116)
- 1986-04-28: SCAN TOOL WORKSHOP ALL 1986 VEHICLES (86-6-114)
- 1986-04-23: METRI-PACK 150 TERMINAL TERMINAL REMOVAL INSTRUCTION (86-B-83)
- 1986-04-23: METRI-PACK 150 TERMINAL TERMINAL REMOVAL INSTRUCTION (86-8-124)
- 1986-04-14: ALUMINUM WHEEL REFINISHING ALL MODELS W/ ALUMINUM WHEELS (86-2-129)
- 1986-04-09: FLUID LEAK DETECTION SPEC. FLUID/BLACK LIGHT USE (86-B-72)
- 1986-04-09: FLUID LEAK DETECTION SPEC. FLUID/BLACK LIGHT USE (86-0-108)
- 1986-03-10: INJECTOR FUEL INJECTOR CLEANER TOOL-J35800 (86-6-111)
- 1986-02-26: CONTROL VALVE ASSEMBLY CLEANING/SERVICING - ALL A/T (86-B-47)
- 1986-02-26: CONTROL VALVE ASSEMBLY CLEANING/SERVICING - ALL A/T (86-7-103)
- 1986-02-17: HARSH 1-2 AND 2-3 UP SHIFTS THM 400 (VR-VV) (86-7400-100)
- 1986-01-31: REMANUFACTURED TBI FUEL INJECTORS (APPLICATION) (86-B-49)
- 1986-01-31: REMANUFACTURED TBI FUEL INJECTORS (APPLICATION) (86-6-129)
- 1986-01-23: AUTOMATIC TRANSMISSION IDENTIFICATION INFORMATION (86-B-42)
- 1986-01-23: AUTOMATIC TRANSMISSION IDENTIFICATION INFORMATION (86-7-102)
- 1986-01-13: TANDEM DIAPHRAGM POWER BRAKE BOOSTER ASSEMBLY (86-5-105)
- 1986-01-07: ANTIFREEZE CONCENTRATION EFFECTS ON ALL ENGINES (86-B-48)
- 1986-01-07: ANTIFREEZE CONCENTRATION EFFECTS ON ALL ENGINES (86-600-110)
- 1986-01-02: ENGINE OIL DISCOLORATION OIL LEAK DETECTION (86-B-29)
- 1985-12-23: WORK AREA & EQUIP. REQUIREMENT TO OVERHAUL TRANSMISSIONS (86-7-101)
- 1985-12-02: ALTERNATOR WHINE-LEFT CHANNEL MODIFY GROUND TO RADIO (86-B-64)
- 1985-12-02: ALTERNATOR WHINE-LEFT CHANNEL MODIFY GROUND TO RADIO (86-8-111)
- 1985-11-13: LUBRICATION OF LOCK CYLINDERS PROPER LUBRICANTS/PRECAUTIONS (86-B-43)
- 1985-11-13: LUBRICATION OF LOCK CYLINDERS PROPER LUBRICANTS/PRECAUTIONS (86-2-105)
- 1985-10-29: RECOMMENDED RTV SEALANTS P/N'S AND APPLICATIONS (86-B-28)
- 1985-10-11: DELAYED ENGAGEMENT-CRUISE III MISDIAGNOSED AS MALFUNCTION (86-B-20)
- 1985-10-11: DELAYED ENGAGEMENT-CRUISE III MISDIAGNOSED AS MALFUNCTION (85-9-113)
- 1985-10-07: CRACKED PAINT USING RM HIGH SOLIDS RAPID FILTER (86-2-103)
- 1985-09-01: 1986 NEW PRODUCT SERVICE BULLETIN FORMAT (86-0-100)
- 1985-08-02: CLARIFICATION AND REVISION OF DIAGNOSTIC ROUTINE,C/C SYSTEM (86-B-27)
- 1985-08-02: CLARIFICATION AND REVISION OF DIAGNOSTIC ROUTINE,C/C SYSTEM (85-9-117)
- 1984-12-17: DIAGNOSIS USING ALDL FUEL FLOW ERRORS-INTEGRATOR/BLOCK LEARN (85-6-126)
- 1984-08-13: EMERGENCY PARTS ORDERING PROCEDURE CLARIFICATION (84-B-25)
- 1984-06-27: CARBURETOR VACUUM BREAK TEST PROCEDURE (85-B-64)
- 1984-06-27: CARBURETOR VACUUM BREAK TEST PROCEDURE (85-6-159)