TRUCK IDENTIFICATION VEHICLES/COMPONENTS DESCRIBED. GMC Truck Caballero 1984

For 1990-2009 cars

# TRUCK IDENTIFICATION VEHICLES/COMPONENTS DESCRIBED

#### MODELS: 1984 MODELS

This bulletin has been prepared to assist in identifying 1984 model vehicles and components as described below.

SUBJECT

Vehicle Identification Number ........................

Light Duty Truck Service Parts Identification Sticker

Engines .............................................

Transaxles ...........................................

Transmissions .......................................

Axles .............................. ................

Light Duty (15-35) Truck Vehicle Identification Number

"C", "K", "G", "S" and Caballero trucks display the VIN plate on the left hand side of the instrument panel areas. On P 42 models, the plate is attached to the top of the radiator support, and on Motor Home Chassis P 32, to the dash and toe panel.

Medium Duty Truck Vehicle Identificaiton Number

On Conventional Cabs, the VIN plate is mounted on the left door lock pillar. On School Bus chassis, the plate is attached to the engine side of the cowl. On "P" models, it is located on top of the radiator support panel.

Body Identification Plate

On the GMC Caballero, the body identification plate is located on the upper horizontal surface of the cowl plenum chamber.

Light Duty Truck Service Parts Identification Sticker

A Service Parts Identification Sticker is furnished for I.D. trucks except Caballero. It contains a complete listing of the vehicle identificaiton number (VIN) wheel base and all production options used to assemble the vehicle, such as suspension, body equipment, engine, axle, transmission, tires, etc.

On "C-K" and "S" models, this sticker is attached to the inner glove compartment. For "P" models, it is mailed separately to the dealer. On "G" models, the sticker is located on the inner hood panel surface.

Truck Engine Production Code Explanation

Chevrolet produced engines, except 6.2L diesel will be stamped with a source, production date and engine suffix. Other General Motors produced engines used in GMC vehicles will use a label affixed to the engine assembly.

Chevrolet Engine Production Code

#### Example:

F 12 10 USC - -- -- ---

Source Month Day Engine Code Code Code Type ---- ---- ---- ----

K=GM of Canada 12th Month 10th day F=Flint Motor December T=Tonawanda V=Flint Engine M=GM of Mexico R=Moraine

#### NOTICE: In addition, all 15-35 Series Trucks have a portion of the vehicle identificaiton number stamped near the engine production code, usually near the right hand side of the cylinder case. This identificaiton number consists of the division code, model year, assembly plant designation and vehicle build sequence number.

Example: C C F 1 2 3 4 5 6

The truck engine codes are located as follows:

L4 2.0L 112 CID Rear Wheel Drive

The engine suffix and build date is steel stamped on a horizontal machined surface on the left rear side of the cylinder case under the exhaust manifold.

L5 250 CID

The engine suffix and build date is steel stamped on a horizontal machined surface on the right side of the cylinder case adjacent to the distributor shaft.

V8

305, 350 CID Engines - the code is stamped ont he cylinder case pad immediately forward of the right hand cylinder head.

366, 427, 454 CID Engines - the code is stamped on a pad on the front top center of the cylinder case immediately forward of the inlet manifold.

V8 Diesel

6.2L (379 Cubic In)

Identification label attached to rocker covers.

#### Example:

10 UTW R 0004441 -- --- - ------- Engine Suffix Plant Build Assembly Code Sequence

For product reports use suffix, plant code and sequential number, i.e. UTWR4441.

1984 Light Duty Truck Engine Codes

Displace- Federal and High Alt. California Vehicle ment R.P.O. Auto. Man. Auto. Man. ------- ---- ------ ----- ----- ------ -----

"S" 1.95L LR1 FZJ FZK FZR FZS FZM FZH S-15 2.2L LQ7 UMU FZW Truck 2.0L LQ2 FWA FW8 FWC FWD FKD FKA FK9 FKH 2.8L LR2 FYB FYD FYA FYC FYH FYS FYF FYR FYK FYN FYJ FYM

"T" 2.0L LQ2 FWM FWN FWW FWX T-15 1.95L LR1 FTZ FZU TRUCK 2.8L LR2 FYU FYX FYT FYN FY2 FZH FYY FZF FZ8 FZD FZA FZC

C-K-P 4.8L L25 FTM FTR FTN FTS 15-35 4.1L LE3 FAH FAL FBX FAJ FAK FAN FAB FAD FAC FAM L.D. FAR TRUCK 5.0L LE9 FCD FCH FCN FCC FCF FCK FCM FDD FDH FDN FDC FDF FDK FDM 5.0L LE3 FDA 5.7L LS9 FRC FRF FRB FRD FRA FSH 5.7L LT9 FRM FSD FSB FSA FSF FSC 5.7L LP9 FFB FFA 7.4L LE9 FSD FSF FBK FBH FBJ FBS FBU FBW FBR FBT 6.2L LM6 FHD FHJ FHB FHL FHF FHH FMC (DIESEL) FJB FJH FHF FJF FJC FJM FJR FJN FJK FJJ FJS MILITARY FJA

"G" 5.0L LE9 FCT FDT FCR FCS FDR FDS 15-35 5.0L LE3 FDB VAN 4.1L LE3 FAS FAU FAW FAX FAB FAT FAY FSA FBB FBC 5.7L LS9 FRJ FRK 5.7L LT9 FSJ FSM FSK FSN 6.2L LL4 FHW FHT FHS FHK FHN FHY FHT FHS FHM FHY FHZ

"P" 5.7L LT9 FRN FSS FSR FSW FRR FSW FSZ FST FSY 25-35 FSX L.D. 6.2L LL4 FJX FJY FJT FJU FJW FJX FJY FJT FJU TRUCK FJZ FFN 7.4L LE8 FBS FBU FBR FBT FBD FBF FBK FBH FBJ FBW FBM 4.8L L25 FTB FTC FTD FTA

Displace Canada Pro Vehicle ment Auto. Man DN ------- ---- ----- --- --

"S" 1.95L IZU S-15 2.2L IZU Truck 2.0L CHEV

2.8L CHEV

"T" 2.0L CHEV T-15 1.95L TRUCK 2.8L CHEV

C-K-P 4.8L CHEV 15-35 4.1L CHEV L.D. TRUCK 5.0L CHEV

5.0L CHEV 5.7L CHEV 5.7L T5B T5A CHEV 5.7L CHEV 7.4L CHEV 6.2L FHD FHB DDA

MILITARY

"G" 5.0L CHEV 15-35 5.0L CHEV VAN 4.1L CHEV

5.7L CHEV 5.7L T5C CHEV 6.2L FHW FHT FHK DDA FHS

"P" 5.7L CHEV 25-35 L.D. 6.2L FJX FJY FJT DDA TRUCK FJW 7.4L CHEV

4.8L MEX

1984 MEDIUM DUTY TRUCK ENG. CODES -----------------------------------

ALL STATES CANADA ENG. AUT. MAN. AUT. MAN. MAN. ---- ---- ---- ---- ---- ---- 7.0L ACA, ACB ACF ABF, ABH ABD CHEV L-43

6.0L AAU, AAW AAX ABB, ABC ABC CHEV L-86 AAK, AAT AAM

TRUCK TRANSMISSION PRODUCTION CODE EXPLANATION

Muncie Manual Transmission Production Code Explanation

The production code number contains the source code, model year and build date.

#### EXAMPLE:

N 4 D 10 - - - --

SOURCE CODE MODEL YEAR BUILD MONTH DAY CODE

S-3 Speed 1984 A - Jan. 10th (Saginaw Type) B - Feb. C - March N-4 Speed D - April (117mm) E - May H - June K - July M - Aug. P - Sept. R - Oct. S - Nov. T - Dec.

3 Speed (Saginaw Type)

The code is stamped on the left side of the cam just below the side cover.

Muncie Truck 4 Speed

Stamped on the rear face of the transmission case just below the rear retainer.

New Process 205.207 and 209 Model 4-Wheel Drive Transfer Case

The build date showing the month, day and year along with the Chevrolet part number is on a metal tag attached to the front face of the transfer case at PTO cover.

Warner Gear Four and Five Speed Manual Transmissions

The manual transmission code, part number and serial number, appears on a metal tag attached to an extension housing bolt on the left side (8 o'clock position).

#### EXAMPLE TAG:

Customer P/N 14078525 WA2041 Source Code

Source P/N 13-52-062 21975 Sequential Serial Number

EXAMPLE

W A 20 4 1 - - -- - - SHIFT SOURCE CODE MONTH DAY YEAR CODE ----------- ----- --- ---- ---- W=Warner A - Jan. G - July 20=20th 4=1984 Shift Produced B - Feb. H - Aug. day C - Mar. J - Sept. D - Apr. K - Oct. E - May L - Nov. F - June M - Dec.

Truck Four-Speed Isuzu Transmission (77.5mm)

Right side of bell housing at 3:00 o'clock position five digit ink stamp transmission serial number. Below serial number is five digit date stamp. 4 - Last Digit of Year 04 - Month 01 - Date

THM 700-R4 Automatic Transmission

The identification number is stamped into right rear oil pan rail. The format includes the year, model, Julian build date and shift.

#### EXAMPLE:

4 YA 222 D - -- --- -

Year Model No. Julian Build Date Shift D=Day N=Night

350C Automatic Transmissions

350C transmissions produced by Chevrolet Parma have a production code stamped on the governor cover.

#### EXAMPLE:

B 4 D 10 D - - - -- -

Source Code Model Year Month Produced Day Produced Shift Produced ----------- ---------- -------------- ------------ -------------- B=Parma 1984 A=Jan 10 Day D=1st (THM 350C) B=Feb N=2nd C=March D=April E=Mauy H=June K=July N=Aug. P=Sept. R=Oct. S= Nov. T=Dec.

400-475 Model Turbo Hydra-matic Transmission

The transmission model number and sequance number is stamped on the identification plate located at the right rear extension.

#### Model and Sequence Number Example:

4 CM 5223 - -- ----

#### Model Year Vehicle Application Code Sequence Number

TRUCK TRANSMISSION IDENTIFICATION NUMBER FOR "SERVICE" USAGE

The following system will be used to identify service transmission assemblies domestically produced. This number system applies to complete service transmission assemblies only. Transmission cases are no longer identified. Manufacturing plants will number each service assembly as it is produced. The first letter will designate the GM division which produced the unit. "C" (Chevrolet).

The second letter will indicate the type of unit. "T" (transmission). The number following the letter will designate the model year. "4" (1984). The last five digits specify the service replacement sequence number. The group o numbers to be used by Chevrolet Manufacturing plants are as follows:

PLANT SERIAL SEOUENCE

Chevrolet - Parma transmission Plant 00001 to 14999 Chevrolet - Muncie Transmission Plant 25000 to 99999 Hydra-Matic 00001 to 99999

Hydra-Matic transmissions will be numbered with the letter "H" regardless of the GM division using the transmission.

EXAMPLE: Number CT400175 designates Chevrolet transmission, year and 175th unit produced for service at Parma.

Upon completion of the serial sequence, the plant will re-use the above numbers using a letter prefix, such as A, B or C tp indicate late production transmission; for example:CT2A0001.

1984 TRUCK TRANSMISSION PROGRAM SUMMARY

PROCESSING NUMBER Manual 3-Speed

M62 2.85 = 1 First Gear Ratio Muncie M64 3.50 = 1 First Gear Ratio Muncie Manual 4-Speed MY6 3.09:1 First Gear Ratio, Overdrive New Process M20 6.55:1 First Gear Ratio Muncie M73 4.09:1 First Gear Ratio Isuzu M77 4.07:1 First Gear Ratio Borg Warner Manual 5-Speed MB1 4.03:1 first Gear Ratio, Overdrive Borg Warner MB6 4.03:1 First Gear Ratio, Overdrive Borg Warner Automatic 3-Speed MV9 200C Converter Clutch Willow Run-Hydra-matic MV4 350C Converter Clutch Parma M40 400 Willow Run-Hydra-matic M40 475 Willow Run-Hydra-matic Automatic 4-Speed MD8 700-R4 Converter Clutch, Overdrive Toledo-Hydra-matic

1984 AXLE IDENTIFICATON CODES "G" SERIES (*INDICATES POSITRACTION)

2.29 RATIO 2.41 RATIO ---------- ---------- Ring Ring Code Gear Code Gear ---- ---- ---- ----

2AH 7.50 2AJ 7.50 *2BH 7.50 *2BJ 7.50 6AT 7.50 6AZ 7.50 *6BT 7.50 *6BZ 7.50

2.73 RATIO 3.08 RATIO 3.42 RATIO 3.73 RATIO ----------- ---------- ---------- ----------- RING RING RING RING CODE GEAR CODE GEAR CODE GEAR CODE GEAR ---- ---- ---- ---- ---- ---- ---- ---- 2AB 7.50 2AC 7.50 6AS 7.50 6TF 8.50 *2BB 7.50 *2BC 7.50 *6BS 7.50 *6TR 8.50 6AX 7.50 6AV 7.50 6TE 8.50 *6BX 7.50 *6BV 7.50 *6TP 8.50 6TJ 7.50

LIGHT DUTY TRUCK REAR AXLE IDENTIFICATION

Light Duty Trucks use either Chevrolet, Dana or Rockwell produced rear axle assemblies. See examples of production codes below.

CHEVROLET AXLE

#### EXAMPLE:

TUF G 001 1 --- - --- - AXLE CODE SOURCE CODE DAY CODE SHIFT CODE --------- ------------ -------- ---------- C = Buffalo Jan.1 = 001 1 st Shift G = Gear & Axle K = GM of Canada

Code is stamped on top of right axle tube outboard of carrier.

DANA AXLE

#### EXAMPLE:

603560 - 1 9 29 4 B 4 ----------- - -- - - -

DANA MONTH DAY MODEL SHIFT PRODUCTION P/N CODE CODE YEAR COOE LINE CODE

Code is stamped on rear surface of right axle tube.

The Chevrolet produced axles use a prefix code stamped into the axle tube for axle code identification. Dana produced axles use the same prefix code as the Chevrolet axles, but they display these codes on a strip of tape attached to the outboard end of the axle tube.

1984 "C" 15-36 Rear Axle Identification

Std.Axle L/D Axle Axle Gear Model Code Code Ratio Brake Size Dia. Rating Axle Mfr. ----- ---- ---- ----- ---------- ----- ------- --------- C100 BN3 - 2.5 11 X 2 8.5 3750 DETROIT G&A BR3 CC3 2.73 BS3 CD3 3.08 BT3 CF3 3.42 BU3 BFH 3.73 BW3 - 2.56 11.15 X 2.75 BX3 CJ3 2.73 BY3 AZ3 3.08 BZ3 BA3 3.42 CA3 BFJ 3.73 C100 CK3 CS3 2.73 11 X 2 V8 + CM3 CT3 3.08 M20 BJK BFM 3.73 CN3 CU3 2.73 11.15 X 2.75 CR3 CW3 3.08 BFN BFR 3.73 C20903 BDB - 3.23 11.15 X 2.75 9.5 5700 BBJ BBF 3.42 BCY BFC 3.73 BCZ BJA 4.10 C20903 BDC - #3.23 13 X 2.50 8000 20906 BBK BBH 3.42 (EXC BFA BDA 3.73 LE8) BJC BJB 4.10 BKC BKD 4.56 (W/LE8) BAA - 3.21 10.5 BCA BCB 3.73 BHA BHB 4.10 C20943 BAB - 3.21 7500 BCC BCD 3.73 BMC BHD 4.10 BKA BKB 4.56 C30903 BAC - 3.21 13 X 3.50 30943 BCF BCH 3.73 31003 BHF BHK 4.10 31403 BKM BKN 4.56 C31003 BAD - #3.21 DETROIT G&A 31403 BCS BCJ 3.73 DUAL WHEEL 30943 BHM BHJ 4.10 BKR BKS 4.56 C30903 BFT - 3.73 DANA 30943 BJK - 4.10 DUAL WHEEL BKK - 4.56

# 3.23 RATIO NOT AVAILABLE ON C20906

@ 3.21 RATIO NOT AVAILABLE ON C30943

1984 "K" 15-35 REAR AXLE IDENTIFICATION

STD. AXLE L/D AXLE AXLE GEAR AXLE MODEL CODE CODE RATIO BRAKE SIZE DIA. RATING AXLE MFR. ----- ---- ---- ------ ---------- ----- ------- ---------- K100 BB3 BH3 2.73 11.15 X 2.75 8.5 3750# DETROIT G&A BC3 BJ3 3.08 EX 06 BD3 BK3 3.42 4000# BF3 BM3 3.73

K100 BRA BRB 2.73 V8 + BSA BSB 3.08 M20 CX3 CZ3 3.42 CY3 DA3 3.73 K20903 BDD - 3.23 9.5 5700 BSC BBA 3.42 BCW BFD 3.73 GDL GDK 4.10 BDF - 3.23 13 x 2.50 6000 K20903 BBD BBM 3.42 20906 BCX BFF 3.73 BHK Duo 4.10 K30903 BCK BCM 3.73 13 x 3.50 10.5 7500 30943 BHR BHS 4.10 31003 BKU BKW 4.56 K30943 BCN BCR 3.73 DETROIT G&A 31003 BHT BHU 4.10 DUAL WHEEL 314003 BKX BKY 4.56 K30903 BFT - 3.73 DANA 30943 BJK - 4.10 DUAL WHEEL BKK - 4.56

1984 "G" 15-35 REAR AXLE IDENTIFICATION

STD.AXLE L/D AXLE AXLE GEAR MODEL CODE CODE RATIO BRAKE SIZE DIA. RATING AXLE MFR. ----- ---- ---- ----- ---------- ---- ------- --------- G100 BRC BRF 2.73 11 X 2 8.5 3500# DETROIT G&A BSC BSF 3.08 BBN BBS 3.42 BFU BFX 3.73

G100 BRD BRH 2.73 11.15 X 2.75 G200 BSD BSH 3.08 BBR BBT 3.42 BFW BFY 3.73

G31305-6 HHB HBC 3.73 13 X 2.50 9.5 5700 31303-32 HBD HBF 4.10

G31303-6 HBG HBH 3.23 31332

G31303 HBJ HBK 4.56 31332 BJFF - 4.10 13 X 3.50 9.75 6200 DANA BKF - 4.56

G31603 BJH - 4.10 31632 BKH - 4.56 G31303 BJJ - 4.10 10.5 7500 31603 BKJ - 4.56 31632

1984 "P" 25-35 GEAR AXLE IDENTIFICATION

STD. AXLE L/D AXLE AXLE GEAR MODEL CODE CODE RATIO BRAKE SIZE DIA RATING AXLE MFR. ----- ---- ---- ----- ----------- --- ------ --------- P20842 BYC BFC 3.73 11.15 X 2.75 9.5 5700 DETROIT G & A 21042 BCZ 4.10

BFA BDA 3.73 6000 BJC 4.10 13 X 2.50

P30842 HBL HBM 3.73 10.5 7900 31042 BHW 4.10 31442 BKZ BMA 4.56

HBN HBP 3.73 13 X 3.50 BHX 4.10 BMB BMC 4.56

P30842 BHY 4.10 DETROIT G & A 31042 BMD BMF 4.56 DUAL WHEEL 31442 BNA 5.13* 31842 30832 31132 31432 31832

P30842 TSA 5.29 13.75 X 1.53 12.0 11000 ROCKWELL 31042 DISC DUAL WHEEL 31442

P31432 BKN 4.56 10.5 10000 DANA 31832 BKI 4.88 DUAL WHEEL CNR 5.13

*5.13 RATIO AXLE NOT AVAILABLE ON MOTOR HOME CHASSIS 032 MODELS.

1984 S-T 15 REAR AXLE IDENTIFICATION

STD.AXLE L/D AXLE AXLE GEAR MODEL CODE CODE RATIO BRAKE SIZE DIA. RATING AXLE MFR.

S100 BRJ BRK 2.73 9.5 X 2 7.5 2800 BUFFALO G & A BSK BSM 3.08 BBU BSW 3.42 BUA BUB 3.73 BTA BTB 4.11 BRR* - 2.73

T100 BRM BRW 2.73 2700 BSN BSR 3.08 BBX BBY 3.42 BUC BUD 3.73 BTC BTD 4.11

* ALUMINUM DRUMS, WITH RPO Z07 ONLY.

LIGHT DUTY TRUCK FOUR WHELL DRIVE FRONT AXLE IDENTIFICATION

GMC Light Duty Truckes use either Chevrolet or Dana produced front axle assemblies. Production code explanations are similar to those covered under rear axle identification.

Chevrolet Axles

Code is stamped on top rear section of left axle tube. (Includes axle ratio code.)

DANA AXLES

Code is stamped on forward side of left axle tube. Axle ratio code on tape strip around right axle tube.

1984 "K" 15-35 FRONT AXLE IDENTIFICATION

AXLE CODE MANUAL AUTO HUB HUB AXLE BRAKE GEAR AXLE MODEL LOCKS LOCKS RATIO SYSTEM DIA. RATING AXLE MFR. ----- ----- ----- ----- ------ ---- ------ ---------- K100 HAN HAA 2.73 JB/D5 8.5 3600 DETROIT G & A HAP HAB 3.08 HAR HAC 3.42 HAS HAD 3.73 K200 HAT HAF 3.23 JB/D6 3800 HAU HAG 3.42 HAW HAH 3.73 K200 HD MKB TFA 3.23 JB/D7 MHC TFB 3.42 MBC TBF 3.73 MCD TFD 4.10 K300 TBA* 3.73 JB/D8 9.75 4500 DANA SINGLE TCA* 4.10 WHEEL TDA* 4.56 K300 TBB* 3.73 DUAL TCB* 4.10 WHEEL TDB* 4.56

*K300 ASSEMBLIES DO NOT INCLUDE HUB LOCKS.

1984 "T" 15 FRONT AXLE IDENTIFICATION

#### MODEL AXLE CODE AXLE RATIO GEAR DIA. AXLE MFG. ----- --------- ---------- --------- ---------

T10 GRK 2.73 7.25 DETROIT G & A GRL 3.08 GRM 3.42 GRN 3.73 GRP 4.11

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.