Fastener Tightening Specifications. GMC Truck Export Savana 1999

For 1990-2009 cars

## Fastener Tightening Specifications Unit Repair

#### Fastener Tightening Specifications (Unit Repair 4L60-E)

Application | Specification
--- | ---
Metric | English
Accumulator Cover to Case Bolt | 8.0-14.0 N·m | 6-10 lb ft
Case Extension to Case Bolt | 42.0-48.0 N·m | 35.0-39.4 lb ft
Case Extension to Case Bolt (4WD Shipping) | 11.2-22.6 N·m | 8.3-16.7 lb ft
Converter Housing to Case Screw | 65.0-75.0 N·m | 48-55 lb ft
Cooler Pipe Connector | 35.0-41.0 N·m | 26-30 lb ft
Detent Spring to Valve Body Bolt | 20.0-27.0 N·m | 15-20 lb ft
Forward Accumulator Cover to Valve Body Bolt | 8.0-14.0 N·m | 6-10 lb ft
Line Pressure Plug | 8.0-14.0 N·m | 6-10 lb ft
Manual Shaft to Inside Detent Lever Nut | 27.0-34.0 N·m | 20-25 lb ft
Oil Passage Cover to Case Bolt | 8.0-14.0 N·m | 6-10 lb ft
Park Brake Bracket to Case Bolt | 27.0-34.0 N·m | 20-25 lb ft
Plate to Case Bolt (Shipping) | 27.0-34.0 N·m | 20-25 lb ft
Plate to Converter Bolt (Shipping) | 27.0-34.0 N·m | 20-25 lb ft
Plug Assembly, A/Trans Oil Pan (C/K) | 30-40 N·m | 22.1-29.5 lb ft
Plug Assembly, A/Trans Oil Pan (Y) | 28-32 N·m | 20.7-23.6 lb ft
Pressure Control Solenoid Bracket to Valve Body Bolt | 8.0-14.0 N·m | 6-10 lb ft
Pump Assembly to Case Bolt | 26.0-32.0 N·m | 19-24 lb ft
Pump Cover to Pump Body Bolt | 20.0-27.0 N·m | 15-20 lb ft
Solenoid Assembly to Case Bolt | 8.0-14.0 N·m | 6-10 lb ft
Speed Sensor Retainer Bolt | 10.5-13.5 N·m | 92.9-119.5 lb in
Stud, A/Trans Case Extension (Y-car) | 18.0-22.0 N·m | 13-16 lb ft
Transmission Fluid Pressure Manual Valve Position Switch to Valve Body Bolt | 8.0-14.0 N·m | 6-10 lb ft
Transmission Oil Cooler Pipe Fitting | 35.0-41.0 N·m | 26-30 lb ft
Transmission Oil Pan to Case Bolt | 9.5-13.8 N·m | 7-10 lb ft
Valve Body to Case Bolt | 8.0-14.0 N·m | 6-10 lb ft