Fastener Tightening Specifications. GMC Truck Export Savana 1999

For 1990-2009 cars

## Fastener Tightening Specifications Overhaul

Application | Specification
--- | ---
Metric | English
Accumulator Housing to Valve Body | 11 N·m | 97 lb in
Case Center Support | 44 N·m | 32 lb ft
Control Valve Assembly to Case | 11 N·m | 97 lb in
Cooler Pipe Connector Nut at Case and Radiator | 38 N·m | 28 lb ft
Engine Rear Mount to Transmission Bolt | 44 N·m | 32 lb ft
Engine Rear Support Bracket to Frame Nut | 44 N·m | 32 lb ft
Extension Housing to Case | 34 N·m | 25 lb ft
Flywheel Housing Cover to Transmission | 7 N·m | 62 lb in
Flywheel to Converter | 44 N·m | 32 lb ft
Fourth Clutch | 23 N·m | 17 lb ft
Manual Shaft to Detent Lever Nut | 24 N·m | 18 lb ft
Oil Pan Drain Plug | 34 N·m | 25 lb ft
Oil Pan to Case | 24 N·m | 18 lb ft
Oil Test Hole Plug | 11 N·m | 97 lb in
Parking Pawl Bracket to Case | 24 N·m | 18 lb ft
Pressure Control Solenoid Bracket to Valve Body | 8 N·m | 71 lb in
Pump Assembly to Case | 24 N·m | 18 lb ft
Pump Body to Cover | 24 N·m | 18 lb ft
Rear Servo Cover to Case | 24 N·m | 18 lb ft
Solenoid to Valve Body | 8 N·m | 71 lb in
Speed Sensor and Bracket Assembly to Case | 11 N·m | 97 lb in
Transmission Case to Engine | 44 N·m | 32 lb ft
Valve Body to Case/Lube Pipe | 11 N·m | 97 lb in
Valve Body to Case/PSM | 11 N·m | 97 lb in