Transmission Wiring Harness Removal. GMC Truck Export Savana 2000

For 1990-2009 cars

1. Disconnect the wire harness connectors from the electrical components.
2. Remove the transmission wiring harness assembly (34) from the wiring harness clamps (33).

Notice: If the transmission wiring harness assembly does not need servicing, do not remove the assembly from the case. Excessive force may damage the pass-through connector.

3. Remove the transmission wiring harness assembly (34) from the case. Use a 1-5/16 inch 12-point socket in order to release the pass-through connector retaining clips from the case.